(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(U1C-VSS7-PadP12)")
	(net 2 "unconnected-(U1K-GPIO2_D5_D-PadAF6)")
	(net 3 "unconnected-(U1F-GPIO0_A2_D-PadAG28)")
	(net 4 "unconnected-(U1Q-MIPI_DSI_TX0_D2P{slash}LVDS_TX0_D2P-PadAH14)")
	(net 5 "unconnected-(U1H-GPIO1_D3_U-PadC23)")
	(net 6 "Net-(U1C-VSS8-PadT14)")
	(net 7 "Net-(U1A-AVSS3-PadAB12)")
	(net 8 "unconnected-(U1L-GPIO3_D0_D-PadAB5)")
	(net 9 "unconnected-(U1H-GPIO1_C2_U-PadE22)")
	(net 10 "unconnected-(U1K-GPIO3_C5_D-PadAC2)")
	(net 11 "unconnected-(U1L-GPIO3_C7_D-PadAA6)")
	(net 12 "Net-(U1A-AVSS2-PadAA12)")
	(net 13 "Net-(U1B-VSS2-PadC11)")
	(net 14 "unconnected-(U1Q-MIPI_DSI_TX0_D3P{slash}LVDS_TX0_D3P-PadAH13)")
	(net 15 "unconnected-(U1I-GPIO2_A1_U-PadH27)")
	(net 16 "unconnected-(U1E-AC2-PadB1)")
	(net 17 "Net-(U1C-VSS10-PadAB2)")
	(net 18 "unconnected-(U1K-GPIO3_A5_D-PadAH3)")
	(net 19 "unconnected-(U1F-GPIO0_D0_U-PadAC20)")
	(net 20 "unconnected-(U1S-EDP_TX_D2N-PadM27)")
	(net 21 "unconnected-(U1F-GPIO0_B0_U-PadAD23)")
	(net 22 "unconnected-(U1G-GPIO1_A7_D-PadB20)")
	(net 23 "unconnected-(U1L-GPIO4_A4_D-PadY2)")
	(net 24 "Net-(U1C-VSS9-PadAA23)")
	(net 25 "Net-(U1A-VDD_CPU-PadJ15)")
	(net 26 "unconnected-(U1E-AC18-PadE11)")
	(net 27 "unconnected-(U1L-GPIO4_B2_D-PadV4)")
	(net 28 "Net-(U1D-DDRPHY_VDDQL-PadJ11)")
	(net 29 "unconnected-(U1O-MIPI_CSI_RX_D2N-PadAD11)")
	(net 30 "unconnected-(U1U-USB2_HOST2_DM-PadR1)")
	(net 31 "unconnected-(U1V-PCIE30_TX1P-PadAB28)")
	(net 32 "unconnected-(U1K-GPIO2_D4_D-PadAF5)")
	(net 33 "unconnected-(U1V-PCIE30_RX1P-PadAD28)")
	(net 34 "Net-(U1B-VSS5-PadK12)")
	(net 35 "unconnected-(U1H-VCCIO2-PadH18)")
	(net 36 "Net-(U1L-VCCIO6-PadR9)")
	(net 37 "unconnected-(U1E-DDR_DQ1_A-PadE1)")
	(net 38 "unconnected-(U1J-GPIO2_C5_D-PadF26)")
	(net 39 "unconnected-(U1P-HDMI_TX_D0P-PadAG20)")
	(net 40 "unconnected-(U1F-GPIO0_C2_D-PadAG23)")
	(net 41 "unconnected-(U1E-AC21-PadF7)")
	(net 42 "unconnected-(U1Q-MIPI_DSI_TX0{slash}LVDS_TX0_AVDD_0V9-PadW16)")
	(net 43 "unconnected-(U1H-GPIO1_D4_U-PadA27)")
	(net 44 "Net-(U1A-VDD_NPU-PadM19)")
	(net 45 "unconnected-(U1T-USB3_HOST1_SSTXN{slash}SATA1_TXN{slash}QSGMII_TXN_M0-PadV27)")
	(net 46 "Net-(U1B-VSS1-PadA1)")
	(net 47 "unconnected-(U1T-USB3_AVDD_0V9-PadP22)")
	(net 48 "unconnected-(U1T-USB3_AVDD_3V3-PadM23)")
	(net 49 "Net-(U1A-AVSS4-PadAE27)")
	(net 50 "unconnected-(U1R-MIPI_DSI_TX1_D0N-PadAE18)")
	(net 51 "unconnected-(U1R-MIPI_DSI_TX1_D3P-PadAD12)")
	(net 52 "Net-(U1B-VSS4-PadG17)")
	(net 53 "unconnected-(U1H-GPIO1_C4_U-PadB22)")
	(net 54 "Net-(U1T-MULTI_PHY_AVDD_0V9-PadR20)")
	(net 55 "unconnected-(U1K-GPIO3_C4_D-PadAC3)")
	(net 56 "unconnected-(U1U-USB2_AVDD_3V3-PadP10)")
	(net 57 "unconnected-(U1L-GPIO4_A6_D-PadW2)")
	(net 58 "unconnected-(U1M-GPIO4_C6_D-PadAE8)")
	(net 59 "unconnected-(U1E-DDR_DQ7_A-PadH4)")
	(net 60 "Net-(U1D-DDRPHY_VDDQ-PadH11)")
	(net 61 "unconnected-(U1J-GPIO2_B1_D-PadD26)")
	(net 62 "unconnected-(U1I-GPIO2_A0_U-PadJ23)")
	(net 63 "unconnected-(U1U-USB2_HOST2_DP-PadR2)")
	(net 64 "unconnected-(U1K-GPIO3_B0_D-PadAG2)")
	(net 65 "unconnected-(U1J-GPIO2_C3_D-PadH24)")
	(net 66 "Net-(U1B-VSS6-PadM11)")
	(net 67 "unconnected-(U1E-DDR_ECC_DQ4-PadM7)")
	(net 68 "unconnected-(U1L-GPIO4_B5_D-PadV5)")
	(net 69 "unconnected-(U1H-GPIO1_C3_U-PadB25)")
	(net 70 "unconnected-(U1T-USB3_AVDD_1V8-PadP23)")
	(net 71 "Net-(U1A-VDD_GPU-PadR13)")
	(net 72 "Net-(U1A-AVSS1-PadJ27)")
	(net 73 "unconnected-(U1L-GPIO4_A5_D-PadY1)")
	(net 74 "unconnected-(U1O-MIPI_CSI_RX_CLK0P-PadAG10)")
	(net 75 "unconnected-(U1E-DDR_DQ9_A-PadN2)")
	(net 76 "unconnected-(U1T-PCIE20_REFCLKN-PadV25)")
	(net 77 "Net-(U1B-VSS3-PadF1)")
	(net 78 "unconnected-(U1J-GPIO2_C0_D-PadF24)")
	(net 79 "unconnected-(U1F-GPIO0_D3_D-PadAE26)")
	(net 80 "unconnected-(U1F-PMUPLL_AVDD_0V9-PadV21)")
	(net 81 "unconnected-(U1L-GPIO4_A3_D-PadY3)")
	(net 82 "unconnected-(U1E-DDR_DQS0N_B-PadB11)")
	(net 83 "unconnected-(U1S-EDP_TX_D3N-PadN27)")
	(net 84 "unconnected-(U1M-GPIO4_C5_D-PadAD8)")
	(net 85 "unconnected-(U1F-PMU_VDD_LOGIC_0V9-PadV19)")
	(net 86 "Net-(U1A-VDD_LOGIC-PadL12)")
	(net 87 "unconnected-(U1L-GPIO3_D2_D-PadY7)")
	(net 88 "unconnected-(U1T-USB3_HOST1_DP-PadP24)")
	(net 89 "unconnected-(U1E-DDR_DQ12_A-PadK2)")
	(net 90 "unconnected-(U1T-PCIE20_TXP{slash}SATA2_TXP{slash}QSGMII_TXP_M1-PadW27)")
	(net 91 "unconnected-(U1T-USB3_OTG0_SSTXN{slash}SATA0_TXN-PadT27)")
	(net 92 "unconnected-(U1E-DDR_DQ7_B-PadE14)")
	(net 93 "unconnected-(U1F-GPIO0_B1_U-PadAF24)")
	(net 94 "unconnected-(U1G-GPIO1_A3_D-PadB19)")
	(net 95 "unconnected-(U1E-DDR_DQ10_B-PadA17)")
	(net 96 "Net-(U1P-HDMI_TX_AVDD_0V9-PadV17)")
	(net 97 "unconnected-(U1U-USB2_HOST3_DM-PadT1)")
	(net 98 "unconnected-(U1R-MIPI_DSI_TX1_D2P-PadAD14)")
	(net 99 "unconnected-(U1E-AC1-PadF5)")
	(net 100 "unconnected-(U1K-GPIO3_B6_D-PadAE3)")
	(net 101 "unconnected-(U1E-DDR_RZQ-PadH7)")
	(net 102 "unconnected-(U1F-GPIO0_C3_D-PadAE23)")
	(net 103 "unconnected-(U1L-GPIO3_D3_D-PadAC1)")
	(net 104 "unconnected-(U1E-AC17-PadE6)")
	(net 105 "unconnected-(U1N-SARADC_VIN0-PadB27)")
	(net 106 "unconnected-(U1F-GPIO0_B6_U-PadAA20)")
	(net 107 "unconnected-(U1H-GPIO1_C0_U-PadA25)")
	(net 108 "unconnected-(U1O-MIPI_CSI_RX_D0N-PadAH12)")
	(net 109 "unconnected-(U1F-GPIO0_A0_D-PadAG27)")
	(net 110 "unconnected-(U1E-AC3-PadF4)")
	(net 111 "unconnected-(U1O-MIPI_CSI_RX_CLK1P-PadAG9)")
	(net 112 "unconnected-(U1O-MIPI_CSI_RX_D0P-PadAG12)")
	(net 113 "unconnected-(U1M-GPIO4_C7_U-PadAG8)")
	(net 114 "unconnected-(U1S-EDP_TX_D1P-PadK28)")
	(net 115 "unconnected-(U1J-GPIO2_C1_D-PadG23)")
	(net 116 "unconnected-(U1V-PCIE30_TX0P-PadAA28)")
	(net 117 "unconnected-(U1S-EDP_TX_D3P-PadM28)")
	(net 118 "unconnected-(U1E-DDR_DQ8_B-PadA16)")
	(net 119 "unconnected-(U1E-DDR_DQS1P_A-PadL2)")
	(net 120 "unconnected-(U1G-GPIO1_B0_D-PadD20)")
	(net 121 "unconnected-(U1H-GPIO1_B6_U-PadB24)")
	(net 122 "unconnected-(U1V-PCIE30_REFCLKN_IN-PadAA25)")
	(net 123 "unconnected-(U1S-EDP_TX_D1N-PadL27)")
	(net 124 "unconnected-(U1P-HDMI_TX_CLKN-PadAG19)")
	(net 125 "unconnected-(U1V-PCIE30_RESREF-PadU19)")
	(net 126 "unconnected-(U1I-GPIO1_D6_U-PadJ24)")
	(net 127 "unconnected-(U1K-GPIO2_D0_D-PadAG6)")
	(net 128 "unconnected-(U1E-DDR_ECC_DM-PadP7)")
	(net 129 "unconnected-(U1O-MIPI_CSI_RX_D1P-PadAG11)")
	(net 130 "unconnected-(U1F-PMUPLL_AVSS-PadV20)")
	(net 131 "unconnected-(U1P-HDMI_TX_D2N-PadAH22)")
	(net 132 "unconnected-(U1M-GPIO4_C2_D-PadAF8)")
	(net 133 "unconnected-(U1I-GPIO1_D5_U-PadJ25)")
	(net 134 "unconnected-(U1K-GPIO2_D1_D-PadAD7)")
	(net 135 "unconnected-(U1L-GPIO3_D1_D-PadAB1)")
	(net 136 "unconnected-(U1G-GPIO1_A0_U-PadD18)")
	(net 137 "unconnected-(U1S-EDP_TX_AUXN-PadM25)")
	(net 138 "unconnected-(U1H-GPIO1_D0_D-PadA22)")
	(net 139 "unconnected-(U1E-DDR_DQ3_A-PadD1)")
	(net 140 "unconnected-(U1G-GPIO1_A2_D-PadA19)")
	(net 141 "unconnected-(U1T-USB3_OTG0_SSRXN{slash}SATA0_RXN-PadR27)")
	(net 142 "unconnected-(U1K-GPIO3_B2_D-PadAF2)")
	(net 143 "unconnected-(U1T-MULTI_PHY1_REFCLKN-PadU24)")
	(net 144 "unconnected-(U1E-DDR_DQS0N_A-PadG2)")
	(net 145 "unconnected-(U1L-GPIO4_A0_D-PadAA3)")
	(net 146 "unconnected-(U1E-DDR_DQ11_A-PadL6)")
	(net 147 "unconnected-(U1I-VCCIO3-PadL22)")
	(net 148 "unconnected-(U1T-PCIE20_RXN{slash}SATA2_RXN{slash}QSGMII_RXN_M1-PadY28)")
	(net 149 "unconnected-(U1E-DDR_ECC_DQ5-PadR7)")
	(net 150 "Net-(U1V-PCIE30_AVDD_0V9-PadU20)")
	(net 151 "unconnected-(U1H-GPIO1_C7_D-PadF20)")
	(net 152 "unconnected-(U1L-GPIO4_B6_D-PadU5)")
	(net 153 "unconnected-(U1S-EDP_TX_AVDD_0V9-PadM20)")
	(net 154 "unconnected-(U1T-PCIE20_RXP{slash}SATA2_RXP{slash}QSGMII_RXP_M1-PadY27)")
	(net 155 "unconnected-(U1K-GPIO3_A0_D-PadAH4)")
	(net 156 "unconnected-(U1E-AC7-PadA8)")
	(net 157 "unconnected-(U1E-DDR_DQ5_A-PadJ2)")
	(net 158 "unconnected-(U1J-GPIO2_C2_D-PadF25)")
	(net 159 "unconnected-(U1H-GPIO1_B7_U-PadD21)")
	(net 160 "unconnected-(U1L-GPIO3_D6_D-PadY6)")
	(net 161 "unconnected-(U1N-SARADC_VIN2-PadD24)")
	(net 162 "unconnected-(U1L-GPIO3_D4_D-PadAA1)")
	(net 163 "unconnected-(U1K-GPIO3_C1_D-PadAD1)")
	(net 164 "unconnected-(U1L-GPIO4_B7_D-PadU4)")
	(net 165 "unconnected-(U1E-DDR_DQ14_B-PadD17)")
	(net 166 "unconnected-(U1T-MULTI_PHY1_REFCLKP-PadU25)")
	(net 167 "unconnected-(U1T-USB3_HOST1_SSRXN{slash}SATA1_RXN{slash}QSGMII_RXN_M0-PadU27)")
	(net 168 "unconnected-(U1J-GPIO2_B4_U-PadG27)")
	(net 169 "unconnected-(U1E-DDR_DQ1_B-PadA9)")
	(net 170 "unconnected-(U1K-GPIO3_A7_D-PadAH2)")
	(net 171 "unconnected-(U1T-MULTI_PHY0_REFCLKP-PadR24)")
	(net 172 "unconnected-(U1F-GPIO0_B4_U-PadAB20)")
	(net 173 "unconnected-(U1V-PCIE30_REFCLKP_IN-PadY25)")
	(net 174 "unconnected-(U1J-GPIO2_B7_D-PadH25)")
	(net 175 "unconnected-(U1E-DDR_ECC_DQ1-PadM4)")
	(net 176 "unconnected-(U1M-VCCIO7-PadV12)")
	(net 177 "unconnected-(U1E-DDR_DQ11_B-PadB18)")
	(net 178 "unconnected-(U1V-PCIE30_RX1N-PadAD27)")
	(net 179 "unconnected-(U1P-HDMI_TX_AVDD_1V8-PadW18)")
	(net 180 "unconnected-(U1E-AC19-PadE9)")
	(net 181 "unconnected-(U1E-DDR_DM0_B-PadD14)")
	(net 182 "unconnected-(U1R-MIPI_DSI_TX1_AVDD_0V9-PadW15)")
	(net 183 "unconnected-(U1E-AC11-PadC2)")
	(net 184 "unconnected-(U1G-GPIO1_A6_D-PadC20)")
	(net 185 "unconnected-(U1E-AC22-PadB3)")
	(net 186 "unconnected-(U1F-GPIO0_C5_D-PadAC21)")
	(net 187 "unconnected-(U1R-MIPI_DSI_TX1_D3N-PadAE12)")
	(net 188 "unconnected-(U1E-DDR_DM0_A-PadH5)")
	(net 189 "unconnected-(U1F-SYSPLL_AVSS-PadN11)")
	(net 190 "unconnected-(U1L-GPIO4_B0_D-PadV7)")
	(net 191 "unconnected-(U1E-AC29-PadF11)")
	(net 192 "unconnected-(U1E-DDR_DQS1N_B-PadA15)")
	(net 193 "unconnected-(U1U-USB2_HOST3_DP-PadT2)")
	(net 194 "unconnected-(U1H-GPIO1_C1_U-PadE21)")
	(net 195 "unconnected-(U1Q-MIPI_DSI_TX0_D1P{slash}LVDS_TX0_D1P-PadAH16)")
	(net 196 "unconnected-(U1J-GPIO2_C6_D-PadE26)")
	(net 197 "unconnected-(U1O-MIPI_CSI_RX_D3P-PadAD9)")
	(net 198 "unconnected-(U1N-SARADC_VIN4-PadG21)")
	(net 199 "unconnected-(U1N-OTP_VCC18-PadH20)")
	(net 200 "unconnected-(U1F-SYSPLL_AVDD_0V9-PadP11)")
	(net 201 "unconnected-(U1F-TVSS-PadAB24)")
	(net 202 "unconnected-(U1J-GPIO2_B3_U-PadF28)")
	(net 203 "unconnected-(U1V-PCIE30_RX0N-PadAC27)")
	(net 204 "unconnected-(U1E-DDR_ECC_DQ3-PadR5)")
	(net 205 "unconnected-(U1R-MIPI_DSI_TX1_D1N-PadAC17)")
	(net 206 "unconnected-(U1T-MULTI_PHY_AVDD_1V8-PadR22)")
	(net 207 "unconnected-(U1L-GPIO4_A7_D-PadW1)")
	(net 208 "unconnected-(U1F-GPIO0_C4_D-PadAD21)")
	(net 209 "unconnected-(U1H-GPIO1_D2_U-PadD23)")
	(net 210 "unconnected-(U1V-PCIE30_TX1N-PadAB27)")
	(net 211 "unconnected-(U1N-SARADC_VIN7-PadF21)")
	(net 212 "unconnected-(U1V-PCIE30_AVDD_1V8-PadU22)")
	(net 213 "unconnected-(U1E-DDR_DQ2_B-PadD12)")
	(net 214 "unconnected-(U1R-MIPI_DSI_TX1_CLKP-PadAD15)")
	(net 215 "unconnected-(U1E-DDR_DQ14_A-PadJ7)")
	(net 216 "unconnected-(U1J-GPIO2_A3_U-PadE27)")
	(net 217 "unconnected-(U1F-GPIO0_B2_U-PadAB21)")
	(net 218 "unconnected-(U1K-GPIO3_B7_D-PadAD4)")
	(net 219 "unconnected-(U1T-USB3_OTG0_DM-PadP28)")
	(net 220 "unconnected-(U1T-USB3_HOST1_SSTXP{slash}SATA1_TXP{slash}QSGMII_TXP_M0-PadV28)")
	(net 221 "unconnected-(U1E-DDR_DQ8_A-PadM1)")
	(net 222 "unconnected-(U1K-GPIO2_D6_D-PadAD6)")
	(net 223 "unconnected-(U1O-MIPI_CSI_RX_D2P-PadAE11)")
	(net 224 "unconnected-(U1E-AC13-PadB8)")
	(net 225 "unconnected-(U1F-GPIO0_D1_U-PadAH24)")
	(net 226 "unconnected-(U1E-DDR_DQ9_B-PadB17)")
	(net 227 "unconnected-(U1I-GPIO1_D7_U-PadH26)")
	(net 228 "unconnected-(U1T-MULTI_PHY0_REFCLKN-PadR25)")
	(net 229 "unconnected-(U1E-DDR_ECC_DQS_N-PadP1)")
	(net 230 "unconnected-(U1K-GPIO3_B4_D-PadAE1)")
	(net 231 "unconnected-(U1E-DDR_DQ15_B-PadB14)")
	(net 232 "unconnected-(U1E-DDR_DQ0_A-PadF2)")
	(net 233 "unconnected-(U1K-GPIO3_B1_D-PadAG1)")
	(net 234 "unconnected-(U1L-GPIO3_D7_D-PadY5)")
	(net 235 "unconnected-(U1G-VCCIO1-PadH17)")
	(net 236 "unconnected-(U1E-AC20-PadF8)")
	(net 237 "unconnected-(U1F-GPIO0_C7_D-PadAH25)")
	(net 238 "unconnected-(U1F-PMUPLL_AVDD_1V8-PadY21)")
	(net 239 "unconnected-(U1O-MIPI_CSI_RX_AVDD_1V8-PadY14)")
	(net 240 "unconnected-(U1S-EDP_TX_D0P-PadJ28)")
	(net 241 "unconnected-(U1L-GPIO4_C1_D-PadU2)")
	(net 242 "unconnected-(U1F-GPIO0_C0_D-PadAD22)")
	(net 243 "unconnected-(U1O-MIPI_CSI_RX_D3N-PadAE9)")
	(net 244 "unconnected-(U1E-DDR_DQ4_A-PadJ1)")
	(net 245 "unconnected-(U1G-GPIO1_A1_U-PadE18)")
	(net 246 "unconnected-(U1E-DDR_ECC_DQS_P-PadP2)")
	(net 247 "unconnected-(U1J-VCCIO4-PadJ21)")
	(net 248 "unconnected-(U1I-GPIO2_A2_D-PadH28)")
	(net 249 "unconnected-(U1F-PMUIO1-PadY20)")
	(net 250 "unconnected-(U1D-DDR_AVSS-PadJ8)")
	(net 251 "unconnected-(U1F-GPIO0_D4_D-PadAB23)")
	(net 252 "unconnected-(U1J-GPIO2_B2_U-PadE25)")
	(net 253 "unconnected-(U1T-USB3_OTG0_DP-PadP27)")
	(net 254 "unconnected-(U1O-MIPI_CSI_RX_CLK0N-PadAH10)")
	(net 255 "unconnected-(U1F-SYSPLL_AVDD_1V8-PadN10)")
	(net 256 "unconnected-(U1P-HDMI_TX_D0N-PadAH20)")
	(net 257 "unconnected-(U1M-GPIO4_C3_D-PadAA11)")
	(net 258 "unconnected-(U1N-SARADC_VIN6-PadG20)")
	(net 259 "unconnected-(U1T-USB3_OTG0_SSTXP{slash}SATA0_TXP-PadT28)")
	(net 260 "unconnected-(U1E-AC10-PadD6)")
	(net 261 "unconnected-(U1F-GPIO0_C1_D-PadAF23)")
	(net 262 "unconnected-(U1E-AC6-PadA7)")
	(net 263 "Net-(U1K-VCCIO5-PadV10)")
	(net 264 "unconnected-(U1R-MIPI_DSI_TX1_D1P-PadAD17)")
	(net 265 "unconnected-(U1Q-MIPI_DSI_TX0_CLKP{slash}LVDS_TX0_CLKP-PadAH15)")
	(net 266 "unconnected-(U1E-DDR_DQ6_B-PadE15)")
	(net 267 "unconnected-(U1K-GPIO3_B5_D-PadAE2)")
	(net 268 "unconnected-(U1Q-MIPI_DSI_TX0_D0N{slash}LVDS_TX0_D0N-PadAG17)")
	(net 269 "unconnected-(U1E-AC5-PadB7)")
	(net 270 "unconnected-(U1L-GPIO4_A2_D-PadY4)")
	(net 271 "unconnected-(U1G-GPIO1_A4_D-PadF18)")
	(net 272 "unconnected-(U1K-GPIO3_A6_D-PadAG3)")
	(net 273 "unconnected-(U1L-GPIO4_B4_D-PadV6)")
	(net 274 "unconnected-(U1J-GPIO2_A5_U-PadB28)")
	(net 275 "unconnected-(U1K-GPIO3_C0_D-PadAD2)")
	(net 276 "unconnected-(U1F-~{POR_U}-PadAH27)")
	(net 277 "unconnected-(U1E-DDR_DQ15_A-PadL4)")
	(net 278 "unconnected-(U1E-AC27-PadE8)")
	(net 279 "unconnected-(U1F-GPIO0_D5_D-PadAD25)")
	(net 280 "unconnected-(U1H-GPIO1_C5_D-PadA23)")
	(net 281 "unconnected-(U1E-AC16-PadD5)")
	(net 282 "unconnected-(U1K-GPIO3_A2_D-PadAE5)")
	(net 283 "unconnected-(U1Q-MIPI_DSI_TX0_D3N{slash}LVDS_TX0_D3N-PadAG13)")
	(net 284 "unconnected-(U1K-GPIO3_C3_D-PadAC4)")
	(net 285 "unconnected-(U1F-GPIO0_B7_D-PadAH26)")
	(net 286 "unconnected-(U1J-GPIO2_A6_U-PadC27)")
	(net 287 "unconnected-(U1K-GPIO2_D3_D-PadAC7)")
	(net 288 "unconnected-(U1H-GPIO1_B4_U-PadA24)")
	(net 289 "unconnected-(U1N-SARADC_AVDD_1V8-PadH22)")
	(net 290 "unconnected-(U1E-DDR_DQS1P_B-PadB15)")
	(net 291 "unconnected-(U1F-XOUT24M-PadAF27)")
	(net 292 "unconnected-(U1E-DDR_DM1_A-PadJ4)")
	(net 293 "unconnected-(U1Q-MIPI_DSI_TX0_D2N{slash}LVDS_TX0_D2N-PadAG14)")
	(net 294 "unconnected-(U1J-GPIO2_B6_U-PadF27)")
	(net 295 "unconnected-(U1E-AC24-PadA4)")
	(net 296 "unconnected-(U1F-GPIO0_A1_Z-PadAG26)")
	(net 297 "unconnected-(U1T-USB3_OTG0_ID-PadL23)")
	(net 298 "unconnected-(U1F-GPIO0_A5_D-PadAF25)")
	(net 299 "unconnected-(U1J-GPIO2_A4_U-PadE28)")
	(net 300 "unconnected-(U1P-HDMI_TX_D1N-PadAH21)")
	(net 301 "unconnected-(U1E-AC12-PadC4)")
	(net 302 "unconnected-(U1Q-MIPI_DSI_TX0_CLKN{slash}LVDS_TX0_CLKN-PadAG15)")
	(net 303 "unconnected-(U1E-AC4-PadD9)")
	(net 304 "unconnected-(U1T-USB3_OTG0_SSRXP{slash}SATA0_RXP-PadR28)")
	(net 305 "unconnected-(U1K-GPIO3_C2_D-PadAA7)")
	(net 306 "unconnected-(U1E-AC23-PadB4)")
	(net 307 "unconnected-(U1L-GPIO4_B3_D-PadV1)")
	(net 308 "unconnected-(U1K-GPIO3_A3_D-PadAG4)")
	(net 309 "unconnected-(U1F-GPIO0_D6_D-PadAC24)")
	(net 310 "unconnected-(U1J-GPIO2_A7_U-PadC28)")
	(net 311 "unconnected-(U1H-GPIO1_C6_D-PadA26)")
	(net 312 "unconnected-(U1H-GPIO1_B5_U-PadC21)")
	(net 313 "unconnected-(U1T-USB3_HOST1_SSRXP{slash}SATA1_RXP{slash}QSGMII_RXP_M0-PadU28)")
	(net 314 "unconnected-(U1S-EDP_TX_AVDD_1V8-PadM22)")
	(net 315 "unconnected-(U1F-GPIO0_C6_D-PadAD20)")
	(net 316 "unconnected-(U1M-GPIO4_D1_U-PadAH6)")
	(net 317 "unconnected-(U1E-AC0-PadB6)")
	(net 318 "unconnected-(U1F-GPIO0_B5_U-PadAC22)")
	(net 319 "unconnected-(U1L-GPIO3_C6_D-PadAC5)")
	(net 320 "unconnected-(U1R-MIPI_DSI_TX1_AVDD_1V8-PadY15)")
	(net 321 "unconnected-(U1J-GPIO2_B0_D-PadD27)")
	(net 322 "unconnected-(U1M-GPIO4_D2_D-PadAB9)")
	(net 323 "unconnected-(U1P-HDMI_TX_REXT-PadAA18)")
	(net 324 "unconnected-(U1K-GPIO2_D2_D-PadAC8)")
	(net 325 "unconnected-(U1S-EDP_TX_AUXP-PadL25)")
	(net 326 "unconnected-(U1E-DDR_DQ10_A-PadL7)")
	(net 327 "unconnected-(U1F-GPIO0_A4_U-PadY22)")
	(net 328 "unconnected-(U1M-GPIO4_D0_U-PadAG7)")
	(net 329 "unconnected-(U1E-DDR_ECC_DQ7-PadR4)")
	(net 330 "unconnected-(U1G-GPIO1_B1_D-PadE20)")
	(net 331 "unconnected-(U1F-PMUIO2-PadW19)")
	(net 332 "unconnected-(U1H-GPIO1_D1_U-PadC24)")
	(net 333 "unconnected-(U1E-DDR_DQ5_B-PadD15)")
	(net 334 "unconnected-(U1Q-MIPI_DSI_TX0_D1N{slash}LVDS_TX0_D1N-PadAG16)")
	(net 335 "unconnected-(U1F-GPIO0_A7_U-PadAG25)")
	(net 336 "unconnected-(U1F-GPIO0_A6_D-PadAE24)")
	(net 337 "unconnected-(U1E-DDR_DQ13_B-PadA13)")
	(net 338 "unconnected-(U1P-HDMI_TX_HPDIN-PadAB18)")
	(net 339 "unconnected-(U1E-AC28-PadD8)")
	(net 340 "unconnected-(U1E-DDR_DQS0P_B-PadA11)")
	(net 341 "unconnected-(U1E-AC9-PadA5)")
	(net 342 "unconnected-(U1E-DDR_VREFOUT-PadP8)")
	(net 343 "unconnected-(U1L-GPIO4_A1_D-PadAA2)")
	(net 344 "unconnected-(U1J-GPIO2_B5_U-PadG28)")
	(net 345 "unconnected-(U1G-GPIO1_A5_D-PadA20)")
	(net 346 "unconnected-(U1E-AC26-PadB2)")
	(net 347 "unconnected-(U1N-SARADC_VIN3-PadE23)")
	(net 348 "unconnected-(U1V-PCIE30_TX0N-PadAA27)")
	(net 349 "unconnected-(U1F-XIN24M-PadAF28)")
	(net 350 "unconnected-(U1P-HDMI_TX_D1P-PadAG21)")
	(net 351 "unconnected-(U1E-DDR_DQ13_A-PadJ6)")
	(net 352 "unconnected-(U1U-USB2_AVDD_1V8-PadP9)")
	(net 353 "unconnected-(U1P-HDMI_TX_CLKP-PadAH19)")
	(net 354 "unconnected-(U1E-DDR_DQS1N_A-PadL1)")
	(net 355 "unconnected-(U1L-GPIO4_C0_D-PadU3)")
	(net 356 "unconnected-(U1E-DDR_DQ0_B-PadB10)")
	(net 357 "unconnected-(U1E-DDR_DQ2_A-PadE2)")
	(net 358 "unconnected-(U1E-DDR_DM1_B-PadE17)")
	(net 359 "unconnected-(U1O-MIPI_CSI_RX_D1N-PadAH11)")
	(net 360 "unconnected-(U1M-GPIO4_C4_D-PadAH7)")
	(net 361 "unconnected-(U1E-DDR_ECC_DQ0-PadP5)")
	(net 362 "unconnected-(U1E-AC14-PadC5)")
	(net 363 "unconnected-(U1Q-MIPI_DSI_TX0_D0P{slash}LVDS_TX0_D0P-PadAH17)")
	(net 364 "unconnected-(U1E-AC15-PadE4)")
	(net 365 "unconnected-(U1N-SARADC_VIN5-PadF22)")
	(net 366 "unconnected-(U1F-GPIO0_A3_U-PadAA22)")
	(net 367 "unconnected-(U1K-GPIO3_A4_D-PadAF4)")
	(net 368 "unconnected-(U1E-DDR_DQ3_B-PadE12)")
	(net 369 "unconnected-(U1O-MIPI_CSI_RX_CLK1N-PadAH9)")
	(net 370 "unconnected-(U1E-DDR_ECC_DQ2-PadM5)")
	(net 371 "unconnected-(U1K-GPIO2_D7_D-PadAH5)")
	(net 372 "unconnected-(U1T-PCIE20_REFCLKP-PadV24)")
	(net 373 "unconnected-(U1J-GPIO2_C4_D-PadH23)")
	(net 374 "unconnected-(U1S-EDP_TX_D2P-PadL28)")
	(net 375 "unconnected-(U1E-DDR_DQ4_B-PadA12)")
	(net 376 "unconnected-(U1L-GPIO4_B1_D-PadV2)")
	(net 377 "unconnected-(U1P-HDMI_TX_D2P-PadAG22)")
	(net 378 "unconnected-(U1O-MIPI_CSI_RX_AVDD_0V9-PadW14)")
	(net 379 "unconnected-(U1T-PCIE20_TXN{slash}SATA2_TXN{slash}QSGMII_TXN_M1-PadW28)")
	(net 380 "unconnected-(U1R-MIPI_DSI_TX1_CLKN-PadAE15)")
	(net 381 "unconnected-(U1A-VDD_CPU_COM-PadM15)")
	(net 382 "unconnected-(U1S-EDP_TX_D0N-PadK27)")
	(net 383 "unconnected-(U1E-DDR_ECC_DQ6-PadP4)")
	(net 384 "unconnected-(U1N-SARADC_VIN1-PadC26)")
	(net 385 "unconnected-(U1E-DDR_DQ6_A-PadH1)")
	(net 386 "unconnected-(U1E-DDR_DQS0P_A-PadG1)")
	(net 387 "unconnected-(U1F-GPIO0_B3_U-PadAG24)")
	(net 388 "unconnected-(U1T-USB3_OTG0_VBUSDET-PadM24)")
	(net 389 "unconnected-(U1K-GPIO3_B3_D-PadAF1)")
	(net 390 "unconnected-(U1T-USB3_HOST1_DM-PadP25)")
	(net 391 "unconnected-(U1G-GPIO1_B3_D-PadB21)")
	(net 392 "unconnected-(U1L-GPIO3_D5_D-PadAA5)")
	(net 393 "unconnected-(U1U-USB2_AVDD_0V9-PadR8)")
	(net 394 "unconnected-(U1Q-MIPI_DSI_TX0{slash}LVDS_TX0_AVDD_1V8-PadY17)")
	(net 395 "unconnected-(U1V-PCIE30_RX0P-PadAC28)")
	(net 396 "unconnected-(U1G-GPIO1_B2_D-PadA21)")
	(net 397 "unconnected-(U1E-DDR_DQ12_B-PadB13)")
	(net 398 "unconnected-(U1R-MIPI_DSI_TX1_D2N-PadAC14)")
	(net 399 "unconnected-(U1R-MIPI_DSI_TX1_D0P-PadAD18)")
	(net 400 "unconnected-(U1E-AC25-PadA2)")
	(net 401 "unconnected-(U1E-AC8-PadC1)")
	(net 402 "unconnected-(U1K-GPIO3_A1_D-PadAB8)")
	(footprint "RK3568:BGA636C65P28X28_1900X1900X168"
		(layer "F.Cu")
		(uuid "2d17a607-32fb-456e-9a74-b3756b46b05b")
		(at 143.525 97.025)
		(property "Reference" "U1"
			(at -6.35 -11.43 0)
			(layer "F.SilkS")
			(uuid "3442d0b7-c2a6-4a6f-af8b-edc4801e089b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "RK3568"
			(at 8.89 11.43 0)
			(layer "F.Fab")
			(uuid "972dc813-9f78-47df-8c8f-14c0c9f0d10e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca925a43-ad72-4218-a7b6-292fe576e6b2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7930311b-f289-4f1e-b292-b78f68db34d1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "MF" "Rockchip"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8a82f72e-2592-493e-ae09-d015b38919ef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.68mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fb4ad17d-b643-4d06-bb47-b1ed673511ce")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Package" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9e089961-d354-4995-969a-c8e4fbc5409e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "18d5b463-64a0-479e-9198-c9bcb1be2103")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RK3568/Fuzhou+Rockchip+Electronics+Co/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3891d4e3-024c-4ebf-b420-6ad097d550e7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "STANDARD" "IPC-7351B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3d759723-3307-4ec0-83c0-73e1f1ef2b15")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "PARTREV" "1.3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c69754d2-5e1d-4b52-99d0-83a973a461fa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RK3568/Fuzhou+Rockchip+Electronics+Co/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac77d153-183d-4965-b9ff-21bd0075aa05")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MP" "RK3568"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a45db626-ceee-4d36-a244-b5f3e196088f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description_1" "Quad-core Cortex-A55 up to 2.0GHz"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "61b5bf5b-47f4-41f6-a552-e4598ee50160")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "51f1c5d5-9d46-4fa7-8fad-8ca3896c9a5a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MANUFACTURER" "Rockchip Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "917a5a75-5358-4204-b0c7-4c0ed88df1d2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/f420a8c4-9c4f-4a8b-b7f4-88d486df007e")
		(sheetname "/")
		(sheetfile "mainboard.kicad_sch")
		(attr smd)
		(fp_line
			(start -9.5 -9.5)
			(end -9.5 -4.75)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f80a534e-5111-4bd9-921e-9296955f7749")
		)
		(fp_line
			(start -9.5 -9.5)
			(end -4.75 -9.5)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "994d67c6-99e2-4a83-9870-afded5dda8a7")
		)
		(fp_line
			(start -9.5 4.75)
			(end -9.5 9.5)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e60c1621-1827-4514-9790-767ae9d23690")
		)
		(fp_line
			(start -9.5 9.5)
			(end -4.75 9.5)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "be80763f-66b2-4163-a1d6-7ba5f90c7734")
		)
		(fp_line
			(start 4.75 -9.5)
			(end 9.5 -9.5)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b7a0be1b-633c-4b31-859b-955d824a4f7a")
		)
		(fp_line
			(start 4.75 9.5)
			(end 9.5 9.5)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e27a384d-0cd7-4753-bc76-d7ede65178fd")
		)
		(fp_line
			(start 9.5 -9.5)
			(end 9.5 -4.75)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2435e297-bdcf-4936-b447-ac0dc31da288")
		)
		(fp_line
			(start 9.5 9.5)
			(end 9.5 4.75)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "08318bfb-7982-4a9e-9634-6af87383cf6d")
		)
		(fp_circle
			(center -10 -8.775)
			(end -9.9 -8.775)
			(stroke
				(width 0.2)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "85cd6c77-17c1-4ea4-b06c-56e11e567ff9")
		)
		(fp_line
			(start -10.5 -10.5)
			(end 10.5 -10.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "700f5b94-8f82-4aea-b0af-6a4e714599b4")
		)
		(fp_line
			(start -10.5 10.5)
			(end -10.5 -10.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1a05773a-f4ad-40e4-8323-fb1755652c75")
		)
		(fp_line
			(start 10.5 -10.5)
			(end 10.5 10.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f08e8b0-3514-4f90-9bae-b96536a59e5a")
		)
		(fp_line
			(start 10.5 10.5)
			(end -10.5 10.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "037aaf4f-0e57-4cd2-9790-a0b818b60b0c")
		)
		(fp_line
			(start -9.5 -9.5)
			(end 9.5 -9.5)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bec080bd-8de4-41d5-b656-309563841de5")
		)
		(fp_line
			(start -9.5 9.5)
			(end -9.5 -9.5)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "243d0085-8717-446a-8201-57ab64f5f806")
		)
		(fp_line
			(start 9.5 -9.5)
			(end 9.5 9.5)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f9c5399-4ec5-4cbe-b30b-aede270dbef8")
		)
		(fp_line
			(start 9.5 9.5)
			(end -9.5 9.5)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fdaa6529-3f54-48a3-b82c-d2b539f5a235")
		)
		(fp_circle
			(center -10 -8.775)
			(end -9.9 -8.775)
			(stroke
				(width 0.2)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "60d683e4-5679-453a-8e15-a6ae1ce004b7")
		)
		(pad "A1" smd circle
			(at -8.775 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "efb1d9d9-3b00-4eab-ad70-22575e13a714")
		)
		(pad "A2" smd circle
			(at -8.125 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 400 "unconnected-(U1E-AC25-PadA2)")
			(pinfunction "AC25")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "fef36c52-c0ab-48b5-88e1-9204268adf05")
		)
		(pad "A3" smd circle
			(at -7.475 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c679468c-6093-46f0-a7de-5f4d7e37dffd")
		)
		(pad "A4" smd circle
			(at -6.825 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 295 "unconnected-(U1E-AC24-PadA4)")
			(pinfunction "AC24")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "b0a8f7a8-b92a-4a50-933e-0ad8d2735890")
		)
		(pad "A5" smd circle
			(at -6.175 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 341 "unconnected-(U1E-AC9-PadA5)")
			(pinfunction "AC9")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "cd116c5a-0ac6-4d62-a0a8-c66d211aa4a3")
		)
		(pad "A6" smd circle
			(at -5.525 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "a78ee5e2-e0e0-4d93-8f47-7cdd5865b6d0")
		)
		(pad "A7" smd circle
			(at -4.875 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 262 "unconnected-(U1E-AC6-PadA7)")
			(pinfunction "AC6")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "a1e59d1e-1f3b-43d5-be1f-bdc0b5f4ee94")
		)
		(pad "A8" smd circle
			(at -4.225 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 156 "unconnected-(U1E-AC7-PadA8)")
			(pinfunction "AC7")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "53b703b3-7dab-443b-a20c-a1f8c23df548")
		)
		(pad "A9" smd circle
			(at -3.575 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 169 "unconnected-(U1E-DDR_DQ1_B-PadA9)")
			(pinfunction "DDR_DQ1_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "5ffe203c-a988-4741-84d3-7eb855baffce")
		)
		(pad "A10" smd circle
			(at -2.925 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c22fbc64-b6d2-4bdc-b3da-0de1df2c56a1")
		)
		(pad "A11" smd circle
			(at -2.275 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 340 "unconnected-(U1E-DDR_DQS0P_B-PadA11)")
			(pinfunction "DDR_DQS0P_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ccb63eac-4a5d-42eb-89d8-99488ecc979c")
		)
		(pad "A12" smd circle
			(at -1.625 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 375 "unconnected-(U1E-DDR_DQ4_B-PadA12)")
			(pinfunction "DDR_DQ4_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ee296b9c-8781-4c34-a9f9-334b713b13c7")
		)
		(pad "A13" smd circle
			(at -0.975 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 337 "unconnected-(U1E-DDR_DQ13_B-PadA13)")
			(pinfunction "DDR_DQ13_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c8e44c1d-7b6d-4e33-aaf5-08f2d0d1e1f6")
		)
		(pad "A14" smd circle
			(at -0.325 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c36766ca-33d9-4f6d-8bf3-305d54672d4c")
		)
		(pad "A15" smd circle
			(at 0.325 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 192 "unconnected-(U1E-DDR_DQS1N_B-PadA15)")
			(pinfunction "DDR_DQS1N_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "6e8e6101-d742-4f93-9aa9-5d69667ab307")
		)
		(pad "A16" smd circle
			(at 0.975 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "unconnected-(U1E-DDR_DQ8_B-PadA16)")
			(pinfunction "DDR_DQ8_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "3ab45b89-d995-46c3-b997-65890782e8c9")
		)
		(pad "A17" smd circle
			(at 1.625 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "unconnected-(U1E-DDR_DQ10_B-PadA17)")
			(pinfunction "DDR_DQ10_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "2bec9943-d2dd-4ae5-8540-152e2160880d")
		)
		(pad "A18" smd circle
			(at 2.275 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "226d8a79-92cc-4bb3-84d6-b745fb7b71b2")
		)
		(pad "A19" smd circle
			(at 2.925 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 140 "unconnected-(U1G-GPIO1_A2_D-PadA19)")
			(pinfunction "GPIO1_A2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "48db69b9-a4c6-4826-b73d-b6d287d9dbc9")
		)
		(pad "A20" smd circle
			(at 3.575 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 345 "unconnected-(U1G-GPIO1_A5_D-PadA20)")
			(pinfunction "GPIO1_A5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "d08dd718-b788-4c75-9012-02451fd0a80d")
		)
		(pad "A21" smd circle
			(at 4.225 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 396 "unconnected-(U1G-GPIO1_B2_D-PadA21)")
			(pinfunction "GPIO1_B2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "fbcc2dd7-904e-46b3-aa5e-161b4ced85ce")
		)
		(pad "A22" smd circle
			(at 4.875 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 138 "unconnected-(U1H-GPIO1_D0_D-PadA22)")
			(pinfunction "GPIO1_D0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "486eaea4-89de-4ca8-95a1-336226218252")
		)
		(pad "A23" smd circle
			(at 5.525 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 280 "unconnected-(U1H-GPIO1_C5_D-PadA23)")
			(pinfunction "GPIO1_C5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ac1b9fb4-1ff7-44a1-a3dd-0a3bb521798f")
		)
		(pad "A24" smd circle
			(at 6.175 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 288 "unconnected-(U1H-GPIO1_B4_U-PadA24)")
			(pinfunction "GPIO1_B4_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "adf0d675-d190-42ce-92ac-877f803a2c80")
		)
		(pad "A25" smd circle
			(at 6.825 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 107 "unconnected-(U1H-GPIO1_C0_U-PadA25)")
			(pinfunction "GPIO1_C0_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "317e0aac-39f8-47ee-9dbc-4bcc1711e89b")
		)
		(pad "A26" smd circle
			(at 7.475 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 311 "unconnected-(U1H-GPIO1_C6_D-PadA26)")
			(pinfunction "GPIO1_C6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "bb712e70-84d8-4525-b0ca-7399aaed9583")
		)
		(pad "A27" smd circle
			(at 8.125 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "unconnected-(U1H-GPIO1_D4_U-PadA27)")
			(pinfunction "GPIO1_D4_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "0f740d34-c499-4a58-9f31-86b7d106bc05")
		)
		(pad "A28" smd circle
			(at 8.775 -8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "11557d1b-a094-47a6-ac84-836eeff07735")
		)
		(pad "AA1" smd circle
			(at -8.775 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 162 "unconnected-(U1L-GPIO3_D4_D-PadAA1)")
			(pinfunction "GPIO3_D4_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "5c5824b0-9e64-4840-98db-034a826ab6b8")
		)
		(pad "AA2" smd circle
			(at -8.125 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 343 "unconnected-(U1L-GPIO4_A1_D-PadAA2)")
			(pinfunction "GPIO4_A1_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "cf08ad8d-c3f8-46c1-a036-9b56150936c4")
		)
		(pad "AA3" smd circle
			(at -7.475 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "unconnected-(U1L-GPIO4_A0_D-PadAA3)")
			(pinfunction "GPIO4_A0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "4cf671d1-363e-4107-8ced-728d43421774")
		)
		(pad "AA4" smd circle
			(at -6.825 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "5b777670-01b3-4636-9e3a-cc61ffd8e32b")
		)
		(pad "AA5" smd circle
			(at -6.175 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 392 "unconnected-(U1L-GPIO3_D5_D-PadAA5)")
			(pinfunction "GPIO3_D5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "fa32c85a-ed2f-4a04-8647-e348489f846f")
		)
		(pad "AA6" smd circle
			(at -5.525 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "unconnected-(U1L-GPIO3_C7_D-PadAA6)")
			(pinfunction "GPIO3_C7_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "03eeaba0-e078-4f08-96a2-e81265507c9f")
		)
		(pad "AA7" smd circle
			(at -4.875 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 305 "unconnected-(U1K-GPIO3_C2_D-PadAA7)")
			(pinfunction "GPIO3_C2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "b6a4f85b-4f5e-46ed-bf23-27d1251402db")
		)
		(pad "AA9" smd circle
			(at -3.575 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "1e2ae064-4343-4790-a093-63bab229d7e2")
		)
		(pad "AA11" smd circle
			(at -2.275 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 257 "unconnected-(U1M-GPIO4_C3_D-PadAA11)")
			(pinfunction "GPIO4_C3_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "9e10ceb6-c044-45c3-ae80-93eb843d0d2b")
		)
		(pad "AA12" smd circle
			(at -1.625 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c949ad7b-8bc3-4e72-a0ad-d09004b66fc6")
		)
		(pad "AA14" smd circle
			(at -0.325 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "459021d1-8f04-4ab1-8fef-f5f852de5f90")
		)
		(pad "AA15" smd circle
			(at 0.325 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "46a46c5e-2c79-40b8-a30f-68bcc856a4a3")
		)
		(pad "AA17" smd circle
			(at 1.625 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "1d4093aa-529a-4fd9-a42b-a496831bb763")
		)
		(pad "AA18" smd circle
			(at 2.275 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 323 "unconnected-(U1P-HDMI_TX_REXT-PadAA18)")
			(pinfunction "HDMI_TX_REXT")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(uuid "c11352eb-bcf6-4749-8ffb-94ff8b544773")
		)
		(pad "AA20" smd circle
			(at 3.575 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "unconnected-(U1F-GPIO0_B6_U-PadAA20)")
			(pinfunction "GPIO0_B6_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "3034c125-27b0-4d00-bf8a-20d56099a1e9")
		)
		(pad "AA22" smd circle
			(at 4.875 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 366 "unconnected-(U1F-GPIO0_A3_U-PadAA22)")
			(pinfunction "GPIO0_A3_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "e7872790-3e38-47a6-aba3-eb9dfc657b98")
		)
		(pad "AA23" smd circle
			(at 5.525 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "7c330399-08b2-43d4-a75d-fb8009a7a030")
		)
		(pad "AA24" smd circle
			(at 6.175 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "786e5a44-daf2-4332-a0e4-0023c3c846a0")
		)
		(pad "AA25" smd circle
			(at 6.825 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 122 "unconnected-(U1V-PCIE30_REFCLKN_IN-PadAA25)")
			(pinfunction "PCIE30_REFCLKN_IN")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "3db3dd22-9123-4782-bd6d-7c0bb2dc1cd3")
		)
		(pad "AA26" smd circle
			(at 7.475 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "69636219-a76b-41d4-8056-1cb2266e017b")
		)
		(pad "AA27" smd circle
			(at 8.125 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 348 "unconnected-(U1V-PCIE30_TX0N-PadAA27)")
			(pinfunction "PCIE30_TX0N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "d4f2eed5-8861-48e1-8250-1046a2d0e4ac")
		)
		(pad "AA28" smd circle
			(at 8.775 4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 116 "unconnected-(U1V-PCIE30_TX0P-PadAA28)")
			(pinfunction "PCIE30_TX0P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "394ef0d5-adee-419f-9bbd-239529809fe8")
		)
		(pad "AB1" smd circle
			(at -8.775 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 135 "unconnected-(U1L-GPIO3_D1_D-PadAB1)")
			(pinfunction "GPIO3_D1_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "447a21b9-e0f0-4c7f-be7d-612aea8f3124")
		)
		(pad "AB2" smd circle
			(at -8.125 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(U1C-VSS10-PadAB2)")
			(pinfunction "VSS10")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "08cf285d-3947-4e31-86ca-535a04d1c3dc")
		)
		(pad "AB5" smd circle
			(at -6.175 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "unconnected-(U1L-GPIO3_D0_D-PadAB5)")
			(pinfunction "GPIO3_D0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "02efb04a-243d-4d9b-a1bb-3c802321a562")
		)
		(pad "AB6" smd circle
			(at -5.525 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(U1C-VSS10-PadAB2)")
			(pinfunction "VSS10")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "3b2cf490-3447-4707-9ab3-2ac7ce5eda02")
		)
		(pad "AB8" smd circle
			(at -4.225 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 402 "unconnected-(U1K-GPIO3_A1_D-PadAB8)")
			(pinfunction "GPIO3_A1_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ff79efe6-6e76-414f-aa4e-8bb446258d9e")
		)
		(pad "AB9" smd circle
			(at -3.575 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 322 "unconnected-(U1M-GPIO4_D2_D-PadAB9)")
			(pinfunction "GPIO4_D2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c0eaa936-2e23-4693-ad32-0e0a94b07ab6")
		)
		(pad "AB11" smd circle
			(at -2.275 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "713bd37f-a4c9-4138-a698-7ab555b65cb9")
		)
		(pad "AB12" smd circle
			(at -1.625 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "72d0e540-6c7f-4f84-b858-72e58a6105a2")
		)
		(pad "AB14" smd circle
			(at -0.325 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "11574713-0f05-429e-a7bc-fcb5d08e98f6")
		)
		(pad "AB15" smd circle
			(at 0.325 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "beac33f5-cf9e-42cb-b70b-3370b0f40af4")
		)
		(pad "AB17" smd circle
			(at 1.625 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "b1b531df-4fe0-4f67-a9f1-3b5ff4597520")
		)
		(pad "AB18" smd circle
			(at 2.275 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 338 "unconnected-(U1P-HDMI_TX_HPDIN-PadAB18)")
			(pinfunction "HDMI_TX_HPDIN")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "c905e32b-2f92-44f8-87c6-86ae163db7c8")
		)
		(pad "AB20" smd circle
			(at 3.575 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 172 "unconnected-(U1F-GPIO0_B4_U-PadAB20)")
			(pinfunction "GPIO0_B4_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "60665a3b-3f03-4896-81b1-02da48d85719")
		)
		(pad "AB21" smd circle
			(at 4.225 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 217 "unconnected-(U1F-GPIO0_B2_U-PadAB21)")
			(pinfunction "GPIO0_B2_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "7c04a9bd-88bc-4cc7-a648-231e494c1f0d")
		)
		(pad "AB23" smd circle
			(at 5.525 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 251 "unconnected-(U1F-GPIO0_D4_D-PadAB23)")
			(pinfunction "GPIO0_D4_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "980c77d7-17ea-40d4-af41-0283deff5a54")
		)
		(pad "AB24" smd circle
			(at 6.175 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 201 "unconnected-(U1F-TVSS-PadAB24)")
			(pinfunction "TVSS")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "75369b97-7582-482a-8fe2-2b8aaec2bb13")
		)
		(pad "AB27" smd circle
			(at 8.125 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 210 "unconnected-(U1V-PCIE30_TX1N-PadAB27)")
			(pinfunction "PCIE30_TX1N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "784a2633-92d1-4cdf-b70a-b93243e1eb76")
		)
		(pad "AB28" smd circle
			(at 8.775 4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "unconnected-(U1V-PCIE30_TX1P-PadAB28)")
			(pinfunction "PCIE30_TX1P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "0bb57e90-4128-4cb8-ad04-f69a0b5424ce")
		)
		(pad "AC1" smd circle
			(at -8.775 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "unconnected-(U1L-GPIO3_D3_D-PadAC1)")
			(pinfunction "GPIO3_D3_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "2e88e44a-975c-4486-a27e-0f85aae3e0a8")
		)
		(pad "AC2" smd circle
			(at -8.125 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "unconnected-(U1K-GPIO3_C5_D-PadAC2)")
			(pinfunction "GPIO3_C5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "03ba3d45-0eab-4a0f-a66e-7ffba6baec39")
		)
		(pad "AC3" smd circle
			(at -7.475 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "unconnected-(U1K-GPIO3_C4_D-PadAC3)")
			(pinfunction "GPIO3_C4_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "1966fcf3-0042-4740-80fc-ff0ef9adfd60")
		)
		(pad "AC4" smd circle
			(at -6.825 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 284 "unconnected-(U1K-GPIO3_C3_D-PadAC4)")
			(pinfunction "GPIO3_C3_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ad1cc5b2-f26e-4cad-b416-fc9bf1844711")
		)
		(pad "AC5" smd circle
			(at -6.175 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 319 "unconnected-(U1L-GPIO3_C6_D-PadAC5)")
			(pinfunction "GPIO3_C6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "be5d8ff2-9786-48b6-b10f-3ec6285b69e5")
		)
		(pad "AC7" smd circle
			(at -4.875 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 287 "unconnected-(U1K-GPIO2_D3_D-PadAC7)")
			(pinfunction "GPIO2_D3_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "adef25f2-511b-4eb6-b8be-285e4b17ffc2")
		)
		(pad "AC8" smd circle
			(at -4.225 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 324 "unconnected-(U1K-GPIO2_D2_D-PadAC8)")
			(pinfunction "GPIO2_D2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c121eb31-22f8-4515-a477-fe9808160de7")
		)
		(pad "AC9" smd circle
			(at -3.575 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "e0d39caa-0d5f-4290-af49-b6f0c0f41e4d")
		)
		(pad "AC11" smd circle
			(at -2.275 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ca37f847-3c63-4d7a-bbfd-c840720de94f")
		)
		(pad "AC12" smd circle
			(at -1.625 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "b91b3886-6ef7-46e7-9000-6c04d2a3c528")
		)
		(pad "AC14" smd circle
			(at -0.325 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 398 "unconnected-(U1R-MIPI_DSI_TX1_D2N-PadAC14)")
			(pinfunction "MIPI_DSI_TX1_D2N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "fdc440fa-6dc0-4925-9ce8-01fbfebd2200")
		)
		(pad "AC15" smd circle
			(at 0.325 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "daa0e8b7-5d54-4556-8f76-0b0d25fcd7a2")
		)
		(pad "AC17" smd circle
			(at 1.625 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 205 "unconnected-(U1R-MIPI_DSI_TX1_D1N-PadAC17)")
			(pinfunction "MIPI_DSI_TX1_D1N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "767025df-0d6c-4631-8175-e6a33d693292")
		)
		(pad "AC18" smd circle
			(at 2.275 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c4354f5c-8bed-4711-a978-ce14a846a834")
		)
		(pad "AC20" smd circle
			(at 3.575 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "unconnected-(U1F-GPIO0_D0_U-PadAC20)")
			(pinfunction "GPIO0_D0_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "07dbbad2-7556-466e-bd55-38bfb6f44d9a")
		)
		(pad "AC21" smd circle
			(at 4.225 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 186 "unconnected-(U1F-GPIO0_C5_D-PadAC21)")
			(pinfunction "GPIO0_C5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "68be8135-4e68-42e3-8154-51b75793e25d")
		)
		(pad "AC22" smd circle
			(at 4.875 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 318 "unconnected-(U1F-GPIO0_B5_U-PadAC22)")
			(pinfunction "GPIO0_B5_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "be5ac766-4a3d-4724-a281-ea9b89a26cff")
		)
		(pad "AC24" smd circle
			(at 6.175 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 309 "unconnected-(U1F-GPIO0_D6_D-PadAC24)")
			(pinfunction "GPIO0_D6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "b9d3a6f5-8d8c-4073-84bb-69e94ff065ce")
		)
		(pad "AC25" smd circle
			(at 6.825 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "5c3a2356-3451-4e15-b3a5-e5facc8b5536")
		)
		(pad "AC26" smd circle
			(at 7.475 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "0f067e1b-76d2-4cad-a886-552764a97a54")
		)
		(pad "AC27" smd circle
			(at 8.125 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 203 "unconnected-(U1V-PCIE30_RX0N-PadAC27)")
			(pinfunction "PCIE30_RX0N")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "75a8a6bd-b560-4cd2-8653-2438c6e2e581")
		)
		(pad "AC28" smd circle
			(at 8.775 5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 395 "unconnected-(U1V-PCIE30_RX0P-PadAC28)")
			(pinfunction "PCIE30_RX0P")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "fbc18f38-b1b5-45c2-8640-ae478401c064")
		)
		(pad "AD1" smd circle
			(at -8.775 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 163 "unconnected-(U1K-GPIO3_C1_D-PadAD1)")
			(pinfunction "GPIO3_C1_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "5d8c8812-8cbc-4887-bb1c-347edf852070")
		)
		(pad "AD2" smd circle
			(at -8.125 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 275 "unconnected-(U1K-GPIO3_C0_D-PadAD2)")
			(pinfunction "GPIO3_C0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "aabf3a6d-f72f-4cfb-b299-d91e038d94c4")
		)
		(pad "AD3" smd circle
			(at -7.475 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(U1C-VSS10-PadAB2)")
			(pinfunction "VSS10")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "e772bbfe-2888-4c72-a624-a8d46737b630")
		)
		(pad "AD4" smd circle
			(at -6.825 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 218 "unconnected-(U1K-GPIO3_B7_D-PadAD4)")
			(pinfunction "GPIO3_B7_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "7c28e5c7-7f26-4ef5-9ce3-a91319225fb4")
		)
		(pad "AD6" smd circle
			(at -5.525 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 222 "unconnected-(U1K-GPIO2_D6_D-PadAD6)")
			(pinfunction "GPIO2_D6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "7f77f7cc-e646-4c55-8f38-561576f45069")
		)
		(pad "AD7" smd circle
			(at -4.875 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 134 "unconnected-(U1K-GPIO2_D1_D-PadAD7)")
			(pinfunction "GPIO2_D1_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "4444458d-31fc-4456-a7a1-565cabeef3ff")
		)
		(pad "AD8" smd circle
			(at -4.225 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "unconnected-(U1M-GPIO4_C5_D-PadAD8)")
			(pinfunction "GPIO4_C5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "260639fa-2e05-4fa3-80b5-15998220c5a0")
		)
		(pad "AD9" smd circle
			(at -3.575 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 197 "unconnected-(U1O-MIPI_CSI_RX_D3P-PadAD9)")
			(pinfunction "MIPI_CSI_RX_D3P")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "731b6f27-01a1-4136-b028-b8b437f80ecb")
		)
		(pad "AD11" smd circle
			(at -2.275 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "unconnected-(U1O-MIPI_CSI_RX_D2N-PadAD11)")
			(pinfunction "MIPI_CSI_RX_D2N")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "0a8ee38c-e907-421a-b645-0f08d6fd0a42")
		)
		(pad "AD12" smd circle
			(at -1.625 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "unconnected-(U1R-MIPI_DSI_TX1_D3P-PadAD12)")
			(pinfunction "MIPI_DSI_TX1_D3P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "1427faaf-711a-4e5c-8a8c-135c79c073a8")
		)
		(pad "AD14" smd circle
			(at -0.325 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "unconnected-(U1R-MIPI_DSI_TX1_D2P-PadAD14)")
			(pinfunction "MIPI_DSI_TX1_D2P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "2cff932d-ee8f-4115-8cb9-3350a1bce692")
		)
		(pad "AD15" smd circle
			(at 0.325 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 214 "unconnected-(U1R-MIPI_DSI_TX1_CLKP-PadAD15)")
			(pinfunction "MIPI_DSI_TX1_CLKP")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "7a96cfe2-c746-4ac8-a916-96470427f341")
		)
		(pad "AD17" smd circle
			(at 1.625 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 264 "unconnected-(U1R-MIPI_DSI_TX1_D1P-PadAD17)")
			(pinfunction "MIPI_DSI_TX1_D1P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "a21ab3fb-6828-42ac-9daf-267dcd321d5d")
		)
		(pad "AD18" smd circle
			(at 2.275 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 399 "unconnected-(U1R-MIPI_DSI_TX1_D0P-PadAD18)")
			(pinfunction "MIPI_DSI_TX1_D0P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "fe2dc8d9-53ac-4731-bc4f-4a78babc1a94")
		)
		(pad "AD20" smd circle
			(at 3.575 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 315 "unconnected-(U1F-GPIO0_C6_D-PadAD20)")
			(pinfunction "GPIO0_C6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "bd1936e9-f31c-42d5-a061-dc5ee6633dda")
		)
		(pad "AD21" smd circle
			(at 4.225 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 208 "unconnected-(U1F-GPIO0_C4_D-PadAD21)")
			(pinfunction "GPIO0_C4_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "781aa265-1b85-4255-a01e-92ea9185a60a")
		)
		(pad "AD22" smd circle
			(at 4.875 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 242 "unconnected-(U1F-GPIO0_C0_D-PadAD22)")
			(pinfunction "GPIO0_C0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "8cc5a184-af32-4e7b-a344-74fd32fa12ed")
		)
		(pad "AD23" smd circle
			(at 5.525 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(U1F-GPIO0_B0_U-PadAD23)")
			(pinfunction "GPIO0_B0_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "081bce4c-d2a4-4a60-8452-5f7f48ab7b5b")
		)
		(pad "AD25" smd circle
			(at 6.825 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 279 "unconnected-(U1F-GPIO0_D5_D-PadAD25)")
			(pinfunction "GPIO0_D5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "abcd0b75-3249-4aa9-978d-3f5350e9c885")
		)
		(pad "AD26" smd circle
			(at 7.475 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "4808942c-ab74-476a-88b5-f5aa25056e12")
		)
		(pad "AD27" smd circle
			(at 8.125 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 178 "unconnected-(U1V-PCIE30_RX1N-PadAD27)")
			(pinfunction "PCIE30_RX1N")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "62f06649-638e-44e7-80e3-ef69637beec7")
		)
		(pad "AD28" smd circle
			(at 8.775 6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "unconnected-(U1V-PCIE30_RX1P-PadAD28)")
			(pinfunction "PCIE30_RX1P")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "0bf768a1-fa49-4a71-9633-bb87bef4a562")
		)
		(pad "AE1" smd circle
			(at -8.775 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 230 "unconnected-(U1K-GPIO3_B4_D-PadAE1)")
			(pinfunction "GPIO3_B4_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "8649a85c-6436-4c71-a475-35724090f69d")
		)
		(pad "AE2" smd circle
			(at -8.125 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 267 "unconnected-(U1K-GPIO3_B5_D-PadAE2)")
			(pinfunction "GPIO3_B5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "a3df0633-3db3-4066-afcf-f5ccabbd3231")
		)
		(pad "AE3" smd circle
			(at -7.475 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "unconnected-(U1K-GPIO3_B6_D-PadAE3)")
			(pinfunction "GPIO3_B6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "2de3cc18-3b3e-4bf0-b684-5f43f2e7126e")
		)
		(pad "AE5" smd circle
			(at -6.175 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 282 "unconnected-(U1K-GPIO3_A2_D-PadAE5)")
			(pinfunction "GPIO3_A2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "acbe954d-cb5f-4950-bc27-480546bd73d6")
		)
		(pad "AE6" smd circle
			(at -5.525 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(U1C-VSS10-PadAB2)")
			(pinfunction "VSS10")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "3fd49170-7553-407e-933b-63376fd81ba6")
		)
		(pad "AE8" smd circle
			(at -4.225 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "unconnected-(U1M-GPIO4_C6_D-PadAE8)")
			(pinfunction "GPIO4_C6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "1b1a3611-dade-438d-949f-c006b8a095d0")
		)
		(pad "AE9" smd circle
			(at -3.575 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 243 "unconnected-(U1O-MIPI_CSI_RX_D3N-PadAE9)")
			(pinfunction "MIPI_CSI_RX_D3N")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "8d8ce1fc-01a0-4175-aca4-d43dc0f70b8a")
		)
		(pad "AE11" smd circle
			(at -2.275 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 223 "unconnected-(U1O-MIPI_CSI_RX_D2P-PadAE11)")
			(pinfunction "MIPI_CSI_RX_D2P")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "7f7a33ed-f4ec-4d84-894d-28b233513908")
		)
		(pad "AE12" smd circle
			(at -1.625 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 187 "unconnected-(U1R-MIPI_DSI_TX1_D3N-PadAE12)")
			(pinfunction "MIPI_DSI_TX1_D3N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "6ba397fb-b479-4191-8630-e1828b5f4ae3")
		)
		(pad "AE14" smd circle
			(at -0.325 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "baeeee15-1921-4db5-a54a-596d2b390360")
		)
		(pad "AE15" smd circle
			(at 0.325 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 380 "unconnected-(U1R-MIPI_DSI_TX1_CLKN-PadAE15)")
			(pinfunction "MIPI_DSI_TX1_CLKN")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "f06d8879-8c83-4757-a250-18cec1ca1f83")
		)
		(pad "AE17" smd circle
			(at 1.625 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "1bb710b5-ecf6-4d0f-8992-23d8189f55a6")
		)
		(pad "AE18" smd circle
			(at 2.275 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "unconnected-(U1R-MIPI_DSI_TX1_D0N-PadAE18)")
			(pinfunction "MIPI_DSI_TX1_D0N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "13bd5e70-aefd-48ef-bb75-50ac32f1388d")
		)
		(pad "AE20" smd circle
			(at 3.575 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(U1A-AVSS3-PadAB12)")
			(pinfunction "AVSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "029b20b4-5f20-4ffe-bbb3-27a84ce31c4f")
		)
		(pad "AE21" smd circle
			(at 4.225 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(U1C-VSS10-PadAB2)")
			(pinfunction "VSS10")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "4e4eef5f-e2b0-44d7-8e3b-586deede75a0")
		)
		(pad "AE23" smd circle
			(at 5.525 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "unconnected-(U1F-GPIO0_C3_D-PadAE23)")
			(pinfunction "GPIO0_C3_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "2e63fc59-b669-4458-8213-170d767f5344")
		)
		(pad "AE24" smd circle
			(at 6.175 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 336 "unconnected-(U1F-GPIO0_A6_D-PadAE24)")
			(pinfunction "GPIO0_A6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c8bf0c02-b0c8-45d5-9932-9e9d76da6f9c")
		)
		(pad "AE26" smd circle
			(at 7.475 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "unconnected-(U1F-GPIO0_D3_D-PadAE26)")
			(pinfunction "GPIO0_D3_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "23ed5671-f0a5-4233-b2e2-e0925f3ee80b")
		)
		(pad "AE27" smd circle
			(at 8.125 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "75de8f6f-f41d-4bb6-ab51-643a153f1519")
		)
		(pad "AE28" smd circle
			(at 8.775 6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c9328ce9-4a9c-48bf-b2d1-0ad2d9b63632")
		)
		(pad "AF1" smd circle
			(at -8.775 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 389 "unconnected-(U1K-GPIO3_B3_D-PadAF1)")
			(pinfunction "GPIO3_B3_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "f9890093-5059-497c-9f34-27d8447524dc")
		)
		(pad "AF2" smd circle
			(at -8.125 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 142 "unconnected-(U1K-GPIO3_B2_D-PadAF2)")
			(pinfunction "GPIO3_B2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "49006de3-962c-4e61-b11a-b7affa142d88")
		)
		(pad "AF3" smd circle
			(at -7.475 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(U1C-VSS10-PadAB2)")
			(pinfunction "VSS10")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "07545b3c-fac4-4091-80e4-c955c890f0bd")
		)
		(pad "AF4" smd circle
			(at -6.825 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 367 "unconnected-(U1K-GPIO3_A4_D-PadAF4)")
			(pinfunction "GPIO3_A4_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "e83aedca-f9ed-46fe-972f-308c336067b3")
		)
		(pad "AF5" smd circle
			(at -6.175 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "unconnected-(U1K-GPIO2_D4_D-PadAF5)")
			(pinfunction "GPIO2_D4_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "0bd7e9d1-5294-448d-a7f4-8112d7c28601")
		)
		(pad "AF6" smd circle
			(at -5.525 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "unconnected-(U1K-GPIO2_D5_D-PadAF6)")
			(pinfunction "GPIO2_D5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "001ff934-696f-47de-8c44-c17f7ee9d4a1")
		)
		(pad "AF8" smd circle
			(at -4.225 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 132 "unconnected-(U1M-GPIO4_C2_D-PadAF8)")
			(pinfunction "GPIO4_C2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "440979e5-717f-4ea5-8f95-44d08b08388d")
		)
		(pad "AF9" smd circle
			(at -3.575 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "2fa4b227-a2eb-4f62-99ba-16bf78e11dbc")
		)
		(pad "AF11" smd circle
			(at -2.275 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "adfd508e-da3a-4f11-91c4-78432208f46f")
		)
		(pad "AF12" smd circle
			(at -1.625 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "fa6ee428-6f3f-45be-b809-fe1f46b8da22")
		)
		(pad "AF14" smd circle
			(at -0.325 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "7d00e2d5-7ca6-454b-8380-0303ae07f414")
		)
		(pad "AF15" smd circle
			(at 0.325 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "13af8f80-94ab-4b19-b618-8fa518ea36c9")
		)
		(pad "AF17" smd circle
			(at 1.625 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "8b72752e-652c-419c-b7a7-046cdfc14f12")
		)
		(pad "AF18" smd circle
			(at 2.275 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "da464ae1-64aa-4c48-a5e6-683393ffd508")
		)
		(pad "AF20" smd circle
			(at 3.575 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "4557542e-ded9-422b-8057-6f6825a7e908")
		)
		(pad "AF21" smd circle
			(at 4.225 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "279d7b6f-bef3-4ab9-9ce4-be07e0f7374d")
		)
		(pad "AF23" smd circle
			(at 5.525 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 261 "unconnected-(U1F-GPIO0_C1_D-PadAF23)")
			(pinfunction "GPIO0_C1_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "a1b0eb0d-f102-4add-bead-91a8c1a009d9")
		)
		(pad "AF24" smd circle
			(at 6.175 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "unconnected-(U1F-GPIO0_B1_U-PadAF24)")
			(pinfunction "GPIO0_B1_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "2ac7884f-6611-4c1a-869b-ff79d2a77ae7")
		)
		(pad "AF25" smd circle
			(at 6.825 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 298 "unconnected-(U1F-GPIO0_A5_D-PadAF25)")
			(pinfunction "GPIO0_A5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "b23e6fc2-fab6-4d70-bfc7-70cd8e6de5fc")
		)
		(pad "AF26" smd circle
			(at 7.475 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(U1C-VSS10-PadAB2)")
			(pinfunction "VSS10")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "99da458b-5556-4d2b-8afe-12b8f91fde24")
		)
		(pad "AF27" smd circle
			(at 8.125 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 291 "unconnected-(U1F-XOUT24M-PadAF27)")
			(pinfunction "XOUT24M")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "af139b95-c0cb-47a1-babb-6dd322dad63a")
		)
		(pad "AF28" smd circle
			(at 8.775 7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 349 "unconnected-(U1F-XIN24M-PadAF28)")
			(pinfunction "XIN24M")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "d77d0725-8c3d-4854-a638-f5e09b9d5009")
		)
		(pad "AG1" smd circle
			(at -8.775 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 233 "unconnected-(U1K-GPIO3_B1_D-PadAG1)")
			(pinfunction "GPIO3_B1_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "87497aef-c683-44a6-9077-6a2b7fdbc266")
		)
		(pad "AG2" smd circle
			(at -8.125 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "unconnected-(U1K-GPIO3_B0_D-PadAG2)")
			(pinfunction "GPIO3_B0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "1e4747c1-d418-4ac8-89dc-b56f246f3a8c")
		)
		(pad "AG3" smd circle
			(at -7.475 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 272 "unconnected-(U1K-GPIO3_A6_D-PadAG3)")
			(pinfunction "GPIO3_A6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "a9d7d68b-27e1-43de-9aba-0bf507711d9b")
		)
		(pad "AG4" smd circle
			(at -6.825 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 308 "unconnected-(U1K-GPIO3_A3_D-PadAG4)")
			(pinfunction "GPIO3_A3_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "b989b3a8-e5b1-4906-ac42-2724cb68c18b")
		)
		(pad "AG5" smd circle
			(at -6.175 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(U1C-VSS10-PadAB2)")
			(pinfunction "VSS10")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ef62a693-4865-4bf6-ae3d-9db65a44c94f")
		)
		(pad "AG6" smd circle
			(at -5.525 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "unconnected-(U1K-GPIO2_D0_D-PadAG6)")
			(pinfunction "GPIO2_D0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "41b3276e-4366-4185-a5e1-fc9802ec02dd")
		)
		(pad "AG7" smd circle
			(at -4.875 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 328 "unconnected-(U1M-GPIO4_D0_U-PadAG7)")
			(pinfunction "GPIO4_D0_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c3914723-6228-48f2-967a-f8c941e8196e")
		)
		(pad "AG8" smd circle
			(at -4.225 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "unconnected-(U1M-GPIO4_C7_U-PadAG8)")
			(pinfunction "GPIO4_C7_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "37af22a7-c22c-4057-8e5f-5cf280bf85f8")
		)
		(pad "AG9" smd circle
			(at -3.575 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "unconnected-(U1O-MIPI_CSI_RX_CLK1P-PadAG9)")
			(pinfunction "MIPI_CSI_RX_CLK1P")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "35d0ef22-160f-4aaa-8d3b-6353106d6370")
		)
		(pad "AG10" smd circle
			(at -2.925 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "unconnected-(U1O-MIPI_CSI_RX_CLK0P-PadAG10)")
			(pinfunction "MIPI_CSI_RX_CLK0P")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "213a431c-f4be-43cf-855e-72e6e13c389c")
		)
		(pad "AG11" smd circle
			(at -2.275 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 129 "unconnected-(U1O-MIPI_CSI_RX_D1P-PadAG11)")
			(pinfunction "MIPI_CSI_RX_D1P")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "420b59b5-5f2c-4526-9899-7439184993dd")
		)
		(pad "AG12" smd circle
			(at -1.625 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "unconnected-(U1O-MIPI_CSI_RX_D0P-PadAG12)")
			(pinfunction "MIPI_CSI_RX_D0P")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "35f9d0ad-6afd-49c2-bc29-e8f141219984")
		)
		(pad "AG13" smd circle
			(at -0.975 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 283 "unconnected-(U1Q-MIPI_DSI_TX0_D3N{slash}LVDS_TX0_D3N-PadAG13)")
			(pinfunction "MIPI_DSI_TX0_D3N/LVDS_TX0_D3N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "acc35ebe-b2f5-49b0-af83-f95c31cb55a3")
		)
		(pad "AG14" smd circle
			(at -0.325 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 293 "unconnected-(U1Q-MIPI_DSI_TX0_D2N{slash}LVDS_TX0_D2N-PadAG14)")
			(pinfunction "MIPI_DSI_TX0_D2N/LVDS_TX0_D2N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "af293554-e377-4dcd-a955-a827a3e24eb2")
		)
		(pad "AG15" smd circle
			(at 0.325 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 302 "unconnected-(U1Q-MIPI_DSI_TX0_CLKN{slash}LVDS_TX0_CLKN-PadAG15)")
			(pinfunction "MIPI_DSI_TX0_CLKN/LVDS_TX0_CLKN")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "b375f2b1-b803-4769-93ac-cb73289b315c")
		)
		(pad "AG16" smd circle
			(at 0.975 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 334 "unconnected-(U1Q-MIPI_DSI_TX0_D1N{slash}LVDS_TX0_D1N-PadAG16)")
			(pinfunction "MIPI_DSI_TX0_D1N/LVDS_TX0_D1N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "c781084f-fffe-407c-8a77-49b6c05a3963")
		)
		(pad "AG17" smd circle
			(at 1.625 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 268 "unconnected-(U1Q-MIPI_DSI_TX0_D0N{slash}LVDS_TX0_D0N-PadAG17)")
			(pinfunction "MIPI_DSI_TX0_D0N/LVDS_TX0_D0N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "a436eeb7-b962-491b-9978-b54f5693e75f")
		)
		(pad "AG18" smd circle
			(at 2.275 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d4930d17-98be-44fc-b37a-99ad952dcf08")
		)
		(pad "AG19" smd circle
			(at 2.925 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 124 "unconnected-(U1P-HDMI_TX_CLKN-PadAG19)")
			(pinfunction "HDMI_TX_CLKN")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "409cfab2-d5d8-4bce-8c29-646eb5cf5795")
		)
		(pad "AG20" smd circle
			(at 3.575 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "unconnected-(U1P-HDMI_TX_D0P-PadAG20)")
			(pinfunction "HDMI_TX_D0P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "0e84668e-04da-4543-b444-3e15f0aa2a8e")
		)
		(pad "AG21" smd circle
			(at 4.225 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 350 "unconnected-(U1P-HDMI_TX_D1P-PadAG21)")
			(pinfunction "HDMI_TX_D1P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "d7c20bef-07a3-430a-9dfe-216ba3462a92")
		)
		(pad "AG22" smd circle
			(at 4.875 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 377 "unconnected-(U1P-HDMI_TX_D2P-PadAG22)")
			(pinfunction "HDMI_TX_D2P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "ef93f214-4e88-4481-9bc1-e8cc7daaa08c")
		)
		(pad "AG23" smd circle
			(at 5.525 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "unconnected-(U1F-GPIO0_C2_D-PadAG23)")
			(pinfunction "GPIO0_C2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "0ed7a385-441b-4f51-b9c2-605dab548840")
		)
		(pad "AG24" smd circle
			(at 6.175 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 387 "unconnected-(U1F-GPIO0_B3_U-PadAG24)")
			(pinfunction "GPIO0_B3_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "f6e3b4e0-b107-4fd0-b5fb-0d458119d232")
		)
		(pad "AG25" smd circle
			(at 6.825 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 335 "unconnected-(U1F-GPIO0_A7_U-PadAG25)")
			(pinfunction "GPIO0_A7_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c7958164-f38a-4650-bbd6-5e414d1ff47d")
		)
		(pad "AG26" smd circle
			(at 7.475 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 296 "unconnected-(U1F-GPIO0_A1_Z-PadAG26)")
			(pinfunction "GPIO0_A1_Z")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "b1843858-58aa-45e2-86fc-dabcfe75785f")
		)
		(pad "AG27" smd circle
			(at 8.125 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "unconnected-(U1F-GPIO0_A0_D-PadAG27)")
			(pinfunction "GPIO0_A0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "339813c5-3e36-4c15-a679-dca702222ba3")
		)
		(pad "AG28" smd circle
			(at 8.775 8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "unconnected-(U1F-GPIO0_A2_D-PadAG28)")
			(pinfunction "GPIO0_A2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "009da8e4-5d12-43eb-bd6d-c93fb780e6b3")
		)
		(pad "AH1" smd circle
			(at -8.775 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(U1C-VSS10-PadAB2)")
			(pinfunction "VSS10")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "9446ad12-16bc-4fa5-9f54-b0777420121f")
		)
		(pad "AH2" smd circle
			(at -8.125 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 170 "unconnected-(U1K-GPIO3_A7_D-PadAH2)")
			(pinfunction "GPIO3_A7_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "601f4fb0-8255-473d-adc5-e140f6683f3f")
		)
		(pad "AH3" smd circle
			(at -7.475 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(U1K-GPIO3_A5_D-PadAH3)")
			(pinfunction "GPIO3_A5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "07a29bdf-d3b0-4d1a-ad34-07c314f7e5e4")
		)
		(pad "AH4" smd circle
			(at -6.825 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 155 "unconnected-(U1K-GPIO3_A0_D-PadAH4)")
			(pinfunction "GPIO3_A0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "53b3a3b3-6fe3-420f-8421-85170c21d18c")
		)
		(pad "AH5" smd circle
			(at -6.175 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 371 "unconnected-(U1K-GPIO2_D7_D-PadAH5)")
			(pinfunction "GPIO2_D7_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ebcf6ef7-44f2-4788-901a-4e8ba0fbe050")
		)
		(pad "AH6" smd circle
			(at -5.525 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 316 "unconnected-(U1M-GPIO4_D1_U-PadAH6)")
			(pinfunction "GPIO4_D1_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "bd7057bb-f387-4886-bb23-38a6b90d0735")
		)
		(pad "AH7" smd circle
			(at -4.875 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 360 "unconnected-(U1M-GPIO4_C4_D-PadAH7)")
			(pinfunction "GPIO4_C4_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "e1406c11-6507-438b-b5e3-1fbe5251c57e")
		)
		(pad "AH8" smd circle
			(at -4.225 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(U1C-VSS10-PadAB2)")
			(pinfunction "VSS10")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "620b457b-0a05-4fe9-87ea-66b09e72ce57")
		)
		(pad "AH9" smd circle
			(at -3.575 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 369 "unconnected-(U1O-MIPI_CSI_RX_CLK1N-PadAH9)")
			(pinfunction "MIPI_CSI_RX_CLK1N")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "eaa86602-9c73-43ac-8067-62a8013a4114")
		)
		(pad "AH10" smd circle
			(at -2.925 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 254 "unconnected-(U1O-MIPI_CSI_RX_CLK0N-PadAH10)")
			(pinfunction "MIPI_CSI_RX_CLK0N")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "9a142d3a-10ff-4749-b025-a19e20eca03d")
		)
		(pad "AH11" smd circle
			(at -2.275 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 359 "unconnected-(U1O-MIPI_CSI_RX_D1N-PadAH11)")
			(pinfunction "MIPI_CSI_RX_D1N")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "e049286b-3faa-4381-ae7e-4eddf3e45228")
		)
		(pad "AH12" smd circle
			(at -1.625 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "unconnected-(U1O-MIPI_CSI_RX_D0N-PadAH12)")
			(pinfunction "MIPI_CSI_RX_D0N")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "331dee4e-5b8a-4270-8d67-a2330434c355")
		)
		(pad "AH13" smd circle
			(at -0.975 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(U1Q-MIPI_DSI_TX0_D3P{slash}LVDS_TX0_D3P-PadAH13)")
			(pinfunction "MIPI_DSI_TX0_D3P/LVDS_TX0_D3P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "0656ef76-07fa-46c2-adfe-544ad31662f2")
		)
		(pad "AH14" smd circle
			(at -0.325 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "unconnected-(U1Q-MIPI_DSI_TX0_D2P{slash}LVDS_TX0_D2P-PadAH14)")
			(pinfunction "MIPI_DSI_TX0_D2P/LVDS_TX0_D2P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "016fff07-c379-442f-888c-8e4c617100a8")
		)
		(pad "AH15" smd circle
			(at 0.325 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 265 "unconnected-(U1Q-MIPI_DSI_TX0_CLKP{slash}LVDS_TX0_CLKP-PadAH15)")
			(pinfunction "MIPI_DSI_TX0_CLKP/LVDS_TX0_CLKP")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "a242e78a-6f0e-45d6-beba-ab417ff9d659")
		)
		(pad "AH16" smd circle
			(at 0.975 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 195 "unconnected-(U1Q-MIPI_DSI_TX0_D1P{slash}LVDS_TX0_D1P-PadAH16)")
			(pinfunction "MIPI_DSI_TX0_D1P/LVDS_TX0_D1P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "71b61065-3fcb-426c-8407-b168fe602991")
		)
		(pad "AH17" smd circle
			(at 1.625 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 363 "unconnected-(U1Q-MIPI_DSI_TX0_D0P{slash}LVDS_TX0_D0P-PadAH17)")
			(pinfunction "MIPI_DSI_TX0_D0P/LVDS_TX0_D0P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "e5f08ded-baec-48da-b225-2466ff54b64f")
		)
		(pad "AH18" smd circle
			(at 2.275 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "731fe7d6-e30f-40b8-9953-7472597a655a")
		)
		(pad "AH19" smd circle
			(at 2.925 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 353 "unconnected-(U1P-HDMI_TX_CLKP-PadAH19)")
			(pinfunction "HDMI_TX_CLKP")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "da314496-aecc-46ff-a3d6-572201934c7e")
		)
		(pad "AH20" smd circle
			(at 3.575 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 256 "unconnected-(U1P-HDMI_TX_D0N-PadAH20)")
			(pinfunction "HDMI_TX_D0N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "9dba59e4-ddd8-4dbc-a56f-6ad8318d6c05")
		)
		(pad "AH21" smd circle
			(at 4.225 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 300 "unconnected-(U1P-HDMI_TX_D1N-PadAH21)")
			(pinfunction "HDMI_TX_D1N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "b32053cb-72b6-4c56-9c7b-190228a5d2f7")
		)
		(pad "AH22" smd circle
			(at 4.875 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 131 "unconnected-(U1P-HDMI_TX_D2N-PadAH22)")
			(pinfunction "HDMI_TX_D2N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "4378abcc-b905-4f7e-a3b2-db27eef856cb")
		)
		(pad "AH23" smd circle
			(at 5.525 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(U1A-AVSS4-PadAE27)")
			(pinfunction "AVSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "eb9d33e5-0d85-40dd-a791-ce44d4b2ee56")
		)
		(pad "AH24" smd circle
			(at 6.175 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 225 "unconnected-(U1F-GPIO0_D1_U-PadAH24)")
			(pinfunction "GPIO0_D1_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "804bf7ec-431f-40ab-901f-1be26ce52e7e")
		)
		(pad "AH25" smd circle
			(at 6.825 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 237 "unconnected-(U1F-GPIO0_C7_D-PadAH25)")
			(pinfunction "GPIO0_C7_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "8965ebdf-4f01-4301-b15f-eedcd83ab477")
		)
		(pad "AH26" smd circle
			(at 7.475 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 285 "unconnected-(U1F-GPIO0_B7_D-PadAH26)")
			(pinfunction "GPIO0_B7_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ad893bd2-26c5-4a21-8737-fe1d3a8d76cb")
		)
		(pad "AH27" smd circle
			(at 8.125 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 276 "unconnected-(U1F-~{POR_U}-PadAH27)")
			(pinfunction "~{POR_U}")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "aae63ef9-45a7-4df2-a4e3-b7d88a326227")
		)
		(pad "AH28" smd circle
			(at 8.775 8.775)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(U1C-VSS10-PadAB2)")
			(pinfunction "VSS10")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "e780422e-f174-440d-bd27-dab1f707238e")
		)
		(pad "B1" smd circle
			(at -8.775 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(U1E-AC2-PadB1)")
			(pinfunction "AC2")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "0716516a-b2e7-4b62-8926-959206b88b5e")
		)
		(pad "B2" smd circle
			(at -8.125 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 346 "unconnected-(U1E-AC26-PadB2)")
			(pinfunction "AC26")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "d18a92fd-d038-4202-a7a4-75b34861bca3")
		)
		(pad "B3" smd circle
			(at -7.475 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 185 "unconnected-(U1E-AC22-PadB3)")
			(pinfunction "AC22")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "6888c3f9-947e-4641-993b-6e61c9830492")
		)
		(pad "B4" smd circle
			(at -6.825 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 306 "unconnected-(U1E-AC23-PadB4)")
			(pinfunction "AC23")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "b80be524-ef9c-4ff7-a2ef-b8fc6db3b4d5")
		)
		(pad "B5" smd circle
			(at -6.175 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c869d48f-c2a5-4f44-b5c1-acb46be0287e")
		)
		(pad "B6" smd circle
			(at -5.525 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 317 "unconnected-(U1E-AC0-PadB6)")
			(pinfunction "AC0")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "bd841ec3-ce6a-408f-8b4b-5f7b7a80cc06")
		)
		(pad "B7" smd circle
			(at -4.875 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 269 "unconnected-(U1E-AC5-PadB7)")
			(pinfunction "AC5")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "a4b1361b-5d04-4aa3-b255-ef26e5b67758")
		)
		(pad "B8" smd circle
			(at -4.225 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 224 "unconnected-(U1E-AC13-PadB8)")
			(pinfunction "AC13")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "7feabaf8-380c-4e3a-b23e-95e7b84113f9")
		)
		(pad "B9" smd circle
			(at -3.575 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "bd69497d-ba04-46c0-b691-7de5e7c5dfa1")
		)
		(pad "B10" smd circle
			(at -2.925 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 356 "unconnected-(U1E-DDR_DQ0_B-PadB10)")
			(pinfunction "DDR_DQ0_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "dbc8acf2-f4d4-4087-bc07-d82f749a7790")
		)
		(pad "B11" smd circle
			(at -2.275 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "unconnected-(U1E-DDR_DQS0N_B-PadB11)")
			(pinfunction "DDR_DQS0N_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "25a0652f-d211-4a9f-8a9f-90ae2d59cb13")
		)
		(pad "B12" smd circle
			(at -1.625 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "da224e1b-5b3d-4025-b0f7-bd6f8cb2961a")
		)
		(pad "B13" smd circle
			(at -0.975 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 397 "unconnected-(U1E-DDR_DQ12_B-PadB13)")
			(pinfunction "DDR_DQ12_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "fd6ba822-e525-4876-8703-c2e842dfe050")
		)
		(pad "B14" smd circle
			(at -0.325 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 231 "unconnected-(U1E-DDR_DQ15_B-PadB14)")
			(pinfunction "DDR_DQ15_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "864e211e-eff9-4626-bd12-119bb53c3511")
		)
		(pad "B15" smd circle
			(at 0.325 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 290 "unconnected-(U1E-DDR_DQS1P_B-PadB15)")
			(pinfunction "DDR_DQS1P_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ae7fca55-4cfe-444e-9298-7c4250429d3c")
		)
		(pad "B16" smd circle
			(at 0.975 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "79ceb33a-61c9-426d-bae3-35716bc9e208")
		)
		(pad "B17" smd circle
			(at 1.625 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 226 "unconnected-(U1E-DDR_DQ9_B-PadB17)")
			(pinfunction "DDR_DQ9_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "808aaee3-d890-4c27-92de-f3d710da11e4")
		)
		(pad "B18" smd circle
			(at 2.275 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 177 "unconnected-(U1E-DDR_DQ11_B-PadB18)")
			(pinfunction "DDR_DQ11_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "62f02395-e278-42a8-b8fd-e173c5cd016a")
		)
		(pad "B19" smd circle
			(at 2.925 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "unconnected-(U1G-GPIO1_A3_D-PadB19)")
			(pinfunction "GPIO1_A3_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "2be43d4b-c4c6-480b-b0df-af7b1920ceb7")
		)
		(pad "B20" smd circle
			(at 3.575 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "unconnected-(U1G-GPIO1_A7_D-PadB20)")
			(pinfunction "GPIO1_A7_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "08b7f053-5e1d-4ca8-980c-145a29d83cdb")
		)
		(pad "B21" smd circle
			(at 4.225 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 391 "unconnected-(U1G-GPIO1_B3_D-PadB21)")
			(pinfunction "GPIO1_B3_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "f9d9a172-27b5-4488-96e2-ad93cbc4d873")
		)
		(pad "B22" smd circle
			(at 4.875 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "unconnected-(U1H-GPIO1_C4_U-PadB22)")
			(pinfunction "GPIO1_C4_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "18546b9f-0d9e-470c-935d-21d064f4d3f7")
		)
		(pad "B23" smd circle
			(at 5.525 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "972eeb4a-2f97-4b6f-89bd-7b935bde06e2")
		)
		(pad "B24" smd circle
			(at 6.175 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 121 "unconnected-(U1H-GPIO1_B6_U-PadB24)")
			(pinfunction "GPIO1_B6_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "3d4a34af-0fd4-47cb-8817-7bbf294e9c0f")
		)
		(pad "B25" smd circle
			(at 6.825 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "unconnected-(U1H-GPIO1_C3_U-PadB25)")
			(pinfunction "GPIO1_C3_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "1f9e21a1-2fb7-4ed7-a608-a5829fe6ed3d")
		)
		(pad "B26" smd circle
			(at 7.475 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "91a2e981-7a55-4b93-9211-dfafcee4133a")
		)
		(pad "B27" smd circle
			(at 8.125 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "unconnected-(U1N-SARADC_VIN0-PadB27)")
			(pinfunction "SARADC_VIN0")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "2fa75b7a-f0d2-4bdb-9439-fbcd2333e2f7")
		)
		(pad "B28" smd circle
			(at 8.775 -8.125)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 274 "unconnected-(U1J-GPIO2_A5_U-PadB28)")
			(pinfunction "GPIO2_A5_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "aa42fe61-4138-4516-93d1-236dc24bb7fc")
		)
		(pad "C1" smd circle
			(at -8.775 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 401 "unconnected-(U1E-AC8-PadC1)")
			(pinfunction "AC8")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "ff2e0793-5c96-4088-96aa-58a7254438b4")
		)
		(pad "C2" smd circle
			(at -8.125 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 183 "unconnected-(U1E-AC11-PadC2)")
			(pinfunction "AC11")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "66e71520-b3d2-4d5a-9502-1d51c3ecf781")
		)
		(pad "C3" smd circle
			(at -7.475 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "82688960-fb84-4959-b464-74972431e2c4")
		)
		(pad "C4" smd circle
			(at -6.825 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 301 "unconnected-(U1E-AC12-PadC4)")
			(pinfunction "AC12")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "b36c4818-82ed-4f7b-8372-8365bb8da137")
		)
		(pad "C5" smd circle
			(at -6.175 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 362 "unconnected-(U1E-AC14-PadC5)")
			(pinfunction "AC14")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "e45a41a0-2755-4e97-8cb3-fc4d4f374342")
		)
		(pad "C6" smd circle
			(at -5.525 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U1B-VSS1-PadA1)")
			(pinfunction "VSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "7d067bca-274d-4a5d-bead-bd9d333a100f")
		)
		(pad "C8" smd circle
			(at -4.225 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "294c16c5-04ba-4055-92bb-8d4c1293de2c")
		)
		(pad "C9" smd circle
			(at -3.575 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "7f0275aa-57d9-4e46-b2f3-8ce7cb80c9aa")
		)
		(pad "C11" smd circle
			(at -2.275 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "534fc888-7d66-4888-b77f-c08024503b76")
		)
		(pad "C12" smd circle
			(at -1.625 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "cb9d923a-9e45-462c-962d-c8c2a7a8f668")
		)
		(pad "C14" smd circle
			(at -0.325 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "513d29c0-3669-4a1d-9984-05a40cb75dd4")
		)
		(pad "C15" smd circle
			(at 0.325 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "758c697e-adc6-47b5-a9f1-19876116fe4a")
		)
		(pad "C17" smd circle
			(at 1.625 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "0654bad6-7425-4557-80fd-ce43e1863c09")
		)
		(pad "C18" smd circle
			(at 2.275 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "b165071e-3f43-4bf2-a3c8-d4486942ec6d")
		)
		(pad "C20" smd circle
			(at 3.575 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 184 "unconnected-(U1G-GPIO1_A6_D-PadC20)")
			(pinfunction "GPIO1_A6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "685ffdce-f28c-47af-8b4d-79a4c4ffdcbe")
		)
		(pad "C21" smd circle
			(at 4.225 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 312 "unconnected-(U1H-GPIO1_B5_U-PadC21)")
			(pinfunction "GPIO1_B5_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "bb913dda-e2da-4a46-a0df-1e44c1678ad9")
		)
		(pad "C23" smd circle
			(at 5.525 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "unconnected-(U1H-GPIO1_D3_U-PadC23)")
			(pinfunction "GPIO1_D3_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "024529c5-5c49-48c1-8a19-41910bb92c0a")
		)
		(pad "C24" smd circle
			(at 6.175 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 332 "unconnected-(U1H-GPIO1_D1_U-PadC24)")
			(pinfunction "GPIO1_D1_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c5ea5761-6e87-4f48-881c-f7f3773eaac0")
		)
		(pad "C25" smd circle
			(at 6.825 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c3e32215-d8c4-45f7-84d2-48a84e1fa3bb")
		)
		(pad "C26" smd circle
			(at 7.475 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 384 "unconnected-(U1N-SARADC_VIN1-PadC26)")
			(pinfunction "SARADC_VIN1")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "f32f2df8-cca2-492d-abd8-b9dd7482d6c2")
		)
		(pad "C27" smd circle
			(at 8.125 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 286 "unconnected-(U1J-GPIO2_A6_U-PadC27)")
			(pinfunction "GPIO2_A6_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ad9ec518-c37c-48bc-9caf-559ac4740fc2")
		)
		(pad "C28" smd circle
			(at 8.775 -7.475)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 310 "unconnected-(U1J-GPIO2_A7_U-PadC28)")
			(pinfunction "GPIO2_A7_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "baa5e75b-e42e-4b14-8ee5-e06579c5140d")
		)
		(pad "D1" smd circle
			(at -8.775 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 139 "unconnected-(U1E-DDR_DQ3_A-PadD1)")
			(pinfunction "DDR_DQ3_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "4877d839-3da7-4903-89b4-4b96ff888f2b")
		)
		(pad "D2" smd circle
			(at -8.125 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "783dde36-ee4e-45cd-bb6c-c087143c5e27")
		)
		(pad "D3" smd circle
			(at -7.475 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "33d9307d-82a2-42dd-a53f-4d1b71f039fb")
		)
		(pad "D5" smd circle
			(at -6.175 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 281 "unconnected-(U1E-AC16-PadD5)")
			(pinfunction "AC16")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "ac282508-6130-4e74-a99c-e95cac9ac501")
		)
		(pad "D6" smd circle
			(at -5.525 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 260 "unconnected-(U1E-AC10-PadD6)")
			(pinfunction "AC10")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "a0dc2195-e75e-49fa-981d-5957a4413ff3")
		)
		(pad "D8" smd circle
			(at -4.225 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 339 "unconnected-(U1E-AC28-PadD8)")
			(pinfunction "AC28")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "ca529b11-c4f8-49e4-83b1-e9c63f4f172e")
		)
		(pad "D9" smd circle
			(at -3.575 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "unconnected-(U1E-AC4-PadD9)")
			(pinfunction "AC4")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "b4574215-9e66-4fb5-a5cf-536b920d043e")
		)
		(pad "D11" smd circle
			(at -2.275 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "1cc49905-48e2-49bc-b427-81070830cb8d")
		)
		(pad "D12" smd circle
			(at -1.625 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 213 "unconnected-(U1E-DDR_DQ2_B-PadD12)")
			(pinfunction "DDR_DQ2_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "7a54d7fe-5da0-4859-8cdd-12eceefa0fcf")
		)
		(pad "D14" smd circle
			(at -0.325 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 181 "unconnected-(U1E-DDR_DM0_B-PadD14)")
			(pinfunction "DDR_DM0_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "6560ee3f-16ac-4714-bda3-998ea0b8d60c")
		)
		(pad "D15" smd circle
			(at 0.325 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 333 "unconnected-(U1E-DDR_DQ5_B-PadD15)")
			(pinfunction "DDR_DQ5_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c639de9f-11ae-4e8b-89e1-d9966e0254ea")
		)
		(pad "D17" smd circle
			(at 1.625 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 165 "unconnected-(U1E-DDR_DQ14_B-PadD17)")
			(pinfunction "DDR_DQ14_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "5e1649f7-c096-4335-a7d1-3e12429cd91c")
		)
		(pad "D18" smd circle
			(at 2.275 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 136 "unconnected-(U1G-GPIO1_A0_U-PadD18)")
			(pinfunction "GPIO1_A0_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "451a99fe-8afa-4fc8-b374-f559a63031bc")
		)
		(pad "D20" smd circle
			(at 3.575 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 120 "unconnected-(U1G-GPIO1_B0_D-PadD20)")
			(pinfunction "GPIO1_B0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "3b98c697-f549-48ff-a44e-54b36a94017c")
		)
		(pad "D21" smd circle
			(at 4.225 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 159 "unconnected-(U1H-GPIO1_B7_U-PadD21)")
			(pinfunction "GPIO1_B7_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "558a378e-81dc-4070-8c25-736ffc70e98b")
		)
		(pad "D23" smd circle
			(at 5.525 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 209 "unconnected-(U1H-GPIO1_D2_U-PadD23)")
			(pinfunction "GPIO1_D2_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "78267e9c-df52-4e9a-bf55-2021be86755e")
		)
		(pad "D24" smd circle
			(at 6.175 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 161 "unconnected-(U1N-SARADC_VIN2-PadD24)")
			(pinfunction "SARADC_VIN2")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "5a959f7c-131c-44e7-a1b8-3fe77f87e47b")
		)
		(pad "D26" smd circle
			(at 7.475 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "unconnected-(U1J-GPIO2_B1_D-PadD26)")
			(pinfunction "GPIO2_B1_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "1d2037db-a5fb-4ce8-a3ad-37bb83f0168c")
		)
		(pad "D27" smd circle
			(at 8.125 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 321 "unconnected-(U1J-GPIO2_B0_D-PadD27)")
			(pinfunction "GPIO2_B0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c08b6816-c2b8-4eb0-8dab-162cf435eb00")
		)
		(pad "D28" smd circle
			(at 8.775 -6.825)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "69b2b543-77e0-4bd3-a4d7-c65bfcfd56a2")
		)
		(pad "E1" smd circle
			(at -8.775 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "unconnected-(U1E-DDR_DQ1_A-PadE1)")
			(pinfunction "DDR_DQ1_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "0dafc9c1-c89e-49a5-afd7-94301f180f11")
		)
		(pad "E2" smd circle
			(at -8.125 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 357 "unconnected-(U1E-DDR_DQ2_A-PadE2)")
			(pinfunction "DDR_DQ2_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "dca4aad9-281c-40af-ab63-b555e5928556")
		)
		(pad "E3" smd circle
			(at -7.475 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "6c3eb5b9-ad5a-441c-9663-65246349bd43")
		)
		(pad "E4" smd circle
			(at -6.825 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 364 "unconnected-(U1E-AC15-PadE4)")
			(pinfunction "AC15")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "e62a9230-1006-4e9c-9dbc-58572f6fbc7d")
		)
		(pad "E6" smd circle
			(at -5.525 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "unconnected-(U1E-AC17-PadE6)")
			(pinfunction "AC17")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "2f36dd19-617d-47f9-94ff-6a109f158589")
		)
		(pad "E7" smd circle
			(at -4.875 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(U1B-VSS2-PadC11)")
			(pinfunction "VSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "f6f121d6-45df-4e86-b8fb-6e32000ed880")
		)
		(pad "E8" smd circle
			(at -4.225 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 278 "unconnected-(U1E-AC27-PadE8)")
			(pinfunction "AC27")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "abc987d3-3a17-4b10-b401-720af872f574")
		)
		(pad "E9" smd circle
			(at -3.575 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 180 "unconnected-(U1E-AC19-PadE9)")
			(pinfunction "AC19")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "64212e1f-bf20-4b51-b5cd-b62bf1a23da2")
		)
		(pad "E11" smd circle
			(at -2.275 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "unconnected-(U1E-AC18-PadE11)")
			(pinfunction "AC18")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "0a57e41b-22d5-48bb-bac5-22c1c5cad9a1")
		)
		(pad "E12" smd circle
			(at -1.625 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 368 "unconnected-(U1E-DDR_DQ3_B-PadE12)")
			(pinfunction "DDR_DQ3_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ea48c03d-d980-4a47-9ef5-fe27ff440404")
		)
		(pad "E14" smd circle
			(at -0.325 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "unconnected-(U1E-DDR_DQ7_B-PadE14)")
			(pinfunction "DDR_DQ7_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "2a865524-83f9-4857-961f-1a348651629a")
		)
		(pad "E15" smd circle
			(at 0.325 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 266 "unconnected-(U1E-DDR_DQ6_B-PadE15)")
			(pinfunction "DDR_DQ6_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "a26babdf-358f-423c-967e-0781da2c2f11")
		)
		(pad "E17" smd circle
			(at 1.625 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 358 "unconnected-(U1E-DDR_DM1_B-PadE17)")
			(pinfunction "DDR_DM1_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "dee44dab-80eb-428b-a0a4-c1120656f034")
		)
		(pad "E18" smd circle
			(at 2.275 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 245 "unconnected-(U1G-GPIO1_A1_U-PadE18)")
			(pinfunction "GPIO1_A1_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "8f87586f-7c9a-45e0-ac70-0f3f4ac6a2be")
		)
		(pad "E20" smd circle
			(at 3.575 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 330 "unconnected-(U1G-GPIO1_B1_D-PadE20)")
			(pinfunction "GPIO1_B1_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c48b1d0d-b895-4ee4-8867-cf551cdfad25")
		)
		(pad "E21" smd circle
			(at 4.225 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 194 "unconnected-(U1H-GPIO1_C1_U-PadE21)")
			(pinfunction "GPIO1_C1_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "704073f8-c1b7-4e0c-a87c-99188832738a")
		)
		(pad "E22" smd circle
			(at 4.875 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "unconnected-(U1H-GPIO1_C2_U-PadE22)")
			(pinfunction "GPIO1_C2_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "033a5274-ab54-4981-8652-4e9e864d4cc1")
		)
		(pad "E23" smd circle
			(at 5.525 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 347 "unconnected-(U1N-SARADC_VIN3-PadE23)")
			(pinfunction "SARADC_VIN3")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "d1beb351-fd09-4a6c-a1cb-c4e14bf4c923")
		)
		(pad "E25" smd circle
			(at 6.825 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 252 "unconnected-(U1J-GPIO2_B2_U-PadE25)")
			(pinfunction "GPIO2_B2_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "981853c3-9be6-4cf4-b545-05fbaab69b09")
		)
		(pad "E26" smd circle
			(at 7.475 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 196 "unconnected-(U1J-GPIO2_C6_D-PadE26)")
			(pinfunction "GPIO2_C6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "728d1a4a-ed07-4dcd-ab80-43950ed01eb3")
		)
		(pad "E27" smd circle
			(at 8.125 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 216 "unconnected-(U1J-GPIO2_A3_U-PadE27)")
			(pinfunction "GPIO2_A3_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "7bb642cd-be7d-4fde-9c07-c962d63d1547")
		)
		(pad "E28" smd circle
			(at 8.775 -6.175)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 299 "unconnected-(U1J-GPIO2_A4_U-PadE28)")
			(pinfunction "GPIO2_A4_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "b2bdca85-06e6-4b6e-a1c5-36e05acce735")
		)
		(pad "F1" smd circle
			(at -8.775 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "578c5f39-db31-41e6-a32b-49a8496791a3")
		)
		(pad "F2" smd circle
			(at -8.125 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 232 "unconnected-(U1E-DDR_DQ0_A-PadF2)")
			(pinfunction "DDR_DQ0_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "86f5771e-9b2f-43a8-8ca8-b9080c0de78d")
		)
		(pad "F3" smd circle
			(at -7.475 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "7fe2acbd-7a55-403e-beb1-931c6b48cf73")
		)
		(pad "F4" smd circle
			(at -6.825 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "unconnected-(U1E-AC3-PadF4)")
			(pinfunction "AC3")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "34a6b2d9-a800-4a17-ae2c-7bcb85106d69")
		)
		(pad "F5" smd circle
			(at -6.175 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "unconnected-(U1E-AC1-PadF5)")
			(pinfunction "AC1")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "2d353a47-7a26-41e0-8dcb-9abce4e7d969")
		)
		(pad "F7" smd circle
			(at -4.875 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "unconnected-(U1E-AC21-PadF7)")
			(pinfunction "AC21")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "0edd9956-776a-416f-a540-c17ef121da88")
		)
		(pad "F8" smd circle
			(at -4.225 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 236 "unconnected-(U1E-AC20-PadF8)")
			(pinfunction "AC20")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "894fc81a-bb09-46f2-9e7a-45b59063d196")
		)
		(pad "F9" smd circle
			(at -3.575 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "4ed2c3a7-cd8c-4300-b7b4-9a2231fe0cb1")
		)
		(pad "F11" smd circle
			(at -2.275 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 191 "unconnected-(U1E-AC29-PadF11)")
			(pinfunction "AC29")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "6e7d60fa-3839-4f10-8e9e-c8d444863b26")
		)
		(pad "F12" smd circle
			(at -1.625 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "e1389b95-f54b-4f18-86fa-5261e2a4040e")
		)
		(pad "F14" smd circle
			(at -0.325 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "8c30542e-eba7-4cd0-a3d8-7a3c3c349596")
		)
		(pad "F15" smd circle
			(at 0.325 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "452571dd-0ab4-4d20-b64b-250db8430554")
		)
		(pad "F17" smd circle
			(at 1.625 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d2fe97c0-eeac-4473-b9e8-b1232adbe4fa")
		)
		(pad "F18" smd circle
			(at 2.275 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 271 "unconnected-(U1G-GPIO1_A4_D-PadF18)")
			(pinfunction "GPIO1_A4_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "a999c8ad-5712-433c-8de5-c4ff187f1fdc")
		)
		(pad "F20" smd circle
			(at 3.575 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 151 "unconnected-(U1H-GPIO1_C7_D-PadF20)")
			(pinfunction "GPIO1_C7_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "51eeb3c7-0708-4c10-84af-887a1115fd45")
		)
		(pad "F21" smd circle
			(at 4.225 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 211 "unconnected-(U1N-SARADC_VIN7-PadF21)")
			(pinfunction "SARADC_VIN7")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "797a9d70-874a-4ca0-944b-97154ef6b9da")
		)
		(pad "F22" smd circle
			(at 4.875 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 365 "unconnected-(U1N-SARADC_VIN5-PadF22)")
			(pinfunction "SARADC_VIN5")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "e71bc0f9-0852-4789-919f-907e294f8cff")
		)
		(pad "F24" smd circle
			(at 6.175 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "unconnected-(U1J-GPIO2_C0_D-PadF24)")
			(pinfunction "GPIO2_C0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "2388b4ef-3abf-4f8e-b16b-f2e04c25c265")
		)
		(pad "F25" smd circle
			(at 6.825 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 158 "unconnected-(U1J-GPIO2_C2_D-PadF25)")
			(pinfunction "GPIO2_C2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "55012f26-fe76-4c58-9248-47b936ddd460")
		)
		(pad "F26" smd circle
			(at 7.475 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "unconnected-(U1J-GPIO2_C5_D-PadF26)")
			(pinfunction "GPIO2_C5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "0df21a44-6e65-48ce-87ef-17808a975a1a")
		)
		(pad "F27" smd circle
			(at 8.125 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 294 "unconnected-(U1J-GPIO2_B6_U-PadF27)")
			(pinfunction "GPIO2_B6_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "b0a248dd-30b9-4121-bc82-b20b4bf45417")
		)
		(pad "F28" smd circle
			(at 8.775 -5.525)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 202 "unconnected-(U1J-GPIO2_B3_U-PadF28)")
			(pinfunction "GPIO2_B3_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "75589d70-864c-498b-900e-dadfa9a2e258")
		)
		(pad "G1" smd circle
			(at -8.775 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 386 "unconnected-(U1E-DDR_DQS0P_A-PadG1)")
			(pinfunction "DDR_DQS0P_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "f4953998-2234-4b04-b1d2-3a31d5285e05")
		)
		(pad "G2" smd circle
			(at -8.125 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "unconnected-(U1E-DDR_DQS0N_A-PadG2)")
			(pinfunction "DDR_DQS0N_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "4c2d6584-912c-495b-ae3c-25113be7f6c4")
		)
		(pad "G5" smd circle
			(at -6.175 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "97881f83-1f59-4678-887f-4db295eba171")
		)
		(pad "G6" smd circle
			(at -5.525 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ee059883-f9ae-4055-af02-73e4494eae53")
		)
		(pad "G8" smd circle
			(at -4.225 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "7f2bb347-87c3-41c5-a1ef-24a488b0797d")
		)
		(pad "G9" smd circle
			(at -3.575 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "a651b30b-76ce-4edf-bc64-0dc505195d93")
		)
		(pad "G11" smd circle
			(at -2.275 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "95da0be5-aa22-488a-92cd-2b70edd03a3e")
		)
		(pad "G12" smd circle
			(at -1.625 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d76ab1f6-fcb6-49b9-89ea-c2d142ae6e96")
		)
		(pad "G14" smd circle
			(at -0.325 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "23867dd3-d2ed-465b-ab5b-622193284375")
		)
		(pad "G15" smd circle
			(at 0.325 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U1B-VSS3-PadF1)")
			(pinfunction "VSS3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "b4a83d79-895f-4dd7-8f7c-bd08ad06dce2")
		)
		(pad "G17" smd circle
			(at 1.625 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "3ae6cd5f-80b9-4e2b-85fc-6bd357c7d2af")
		)
		(pad "G18" smd circle
			(at 2.275 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "17ba8dae-778e-4f8b-a2b6-b20dfff854a2")
		)
		(pad "G20" smd circle
			(at 3.575 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 258 "unconnected-(U1N-SARADC_VIN6-PadG20)")
			(pinfunction "SARADC_VIN6")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "9e24b586-717f-4073-b6f8-94118cd88f58")
		)
		(pad "G21" smd circle
			(at 4.225 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 198 "unconnected-(U1N-SARADC_VIN4-PadG21)")
			(pinfunction "SARADC_VIN4")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "73432d9c-7cce-4300-b95a-5b6fbae85e13")
		)
		(pad "G23" smd circle
			(at 5.525 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 115 "unconnected-(U1J-GPIO2_C1_D-PadG23)")
			(pinfunction "GPIO2_C1_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "39286230-e433-46ef-8a6a-2dec49cfee31")
		)
		(pad "G24" smd circle
			(at 6.175 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ff0f9273-9947-4a69-ac47-fadf0b9b7d3c")
		)
		(pad "G27" smd circle
			(at 8.125 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 168 "unconnected-(U1J-GPIO2_B4_U-PadG27)")
			(pinfunction "GPIO2_B4_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "5f682eac-7160-4bfa-b82a-b6ff67bf326f")
		)
		(pad "G28" smd circle
			(at 8.775 -4.875)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 344 "unconnected-(U1J-GPIO2_B5_U-PadG28)")
			(pinfunction "GPIO2_B5_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "d0075991-47ee-4b57-96d0-1a829753ee10")
		)
		(pad "H1" smd circle
			(at -8.775 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 385 "unconnected-(U1E-DDR_DQ6_A-PadH1)")
			(pinfunction "DDR_DQ6_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "f3efd36f-a8af-415e-a5d9-ca39278f65f3")
		)
		(pad "H2" smd circle
			(at -8.125 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c34cc231-f4ad-4161-9a8c-a8effddc20af")
		)
		(pad "H3" smd circle
			(at -7.475 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "2de57a0d-1cb7-4ea5-951b-06cee5126843")
		)
		(pad "H4" smd circle
			(at -6.825 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "unconnected-(U1E-DDR_DQ7_A-PadH4)")
			(pinfunction "DDR_DQ7_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "1b6ddb76-43df-4fc2-82fe-76f9949f9abb")
		)
		(pad "H5" smd circle
			(at -6.175 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 188 "unconnected-(U1E-DDR_DM0_A-PadH5)")
			(pinfunction "DDR_DM0_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "6bba3d86-ea4a-4626-ad1d-4ce9f60b6f09")
		)
		(pad "H6" smd circle
			(at -5.525 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "20f44e1b-57cc-46d7-84e3-4f191247567b")
		)
		(pad "H7" smd circle
			(at -4.875 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "unconnected-(U1E-DDR_RZQ-PadH7)")
			(pinfunction "DDR_RZQ")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(uuid "2e479035-0528-441c-a0cd-8d412aad0c25")
		)
		(pad "H9" smd circle
			(at -3.575 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(U1D-DDRPHY_VDDQ-PadH11)")
			(pinfunction "DDRPHY_VDDQ")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "201499ae-211e-40ac-98f3-42fb5a530760")
		)
		(pad "H11" smd circle
			(at -2.275 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(U1D-DDRPHY_VDDQ-PadH11)")
			(pinfunction "DDRPHY_VDDQ")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "1d1a2a5e-90da-4ac5-b870-f6048b472972")
		)
		(pad "H12" smd circle
			(at -1.625 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(U1D-DDRPHY_VDDQ-PadH11)")
			(pinfunction "DDRPHY_VDDQ")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "2dcbbcbc-7559-4d02-a016-dc861dca2199")
		)
		(pad "H14" smd circle
			(at -0.325 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(U1D-DDRPHY_VDDQ-PadH11)")
			(pinfunction "DDRPHY_VDDQ")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "af8b6177-56a6-4760-86b3-a358cee23aa2")
		)
		(pad "H15" smd circle
			(at 0.325 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(U1D-DDRPHY_VDDQ-PadH11)")
			(pinfunction "DDRPHY_VDDQ")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "aca704f4-649a-472b-9a74-ef1db66970fb")
		)
		(pad "H17" smd circle
			(at 1.625 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 235 "unconnected-(U1G-VCCIO1-PadH17)")
			(pinfunction "VCCIO1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "88885b34-1a7b-4022-a97b-cb6f8b6ec4b3")
		)
		(pad "H18" smd circle
			(at 2.275 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "unconnected-(U1H-VCCIO2-PadH18)")
			(pinfunction "VCCIO2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "0d20966d-f138-48dc-b567-aaf3364c1b5d")
		)
		(pad "H20" smd circle
			(at 3.575 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 199 "unconnected-(U1N-OTP_VCC18-PadH20)")
			(pinfunction "OTP_VCC18")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "73c4009a-205d-4e89-8442-d6ffe0c16206")
		)
		(pad "H22" smd circle
			(at 4.875 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 289 "unconnected-(U1N-SARADC_AVDD_1V8-PadH22)")
			(pinfunction "SARADC_AVDD_1V8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ae60bd38-8b0d-4e37-b941-ee5f91abb691")
		)
		(pad "H23" smd circle
			(at 5.525 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 373 "unconnected-(U1J-GPIO2_C4_D-PadH23)")
			(pinfunction "GPIO2_C4_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ec46d48a-2816-41ed-9124-1f04149c0b46")
		)
		(pad "H24" smd circle
			(at 6.175 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "unconnected-(U1J-GPIO2_C3_D-PadH24)")
			(pinfunction "GPIO2_C3_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "1e726470-23c3-4d15-a699-b39e8db6b830")
		)
		(pad "H25" smd circle
			(at 6.825 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 174 "unconnected-(U1J-GPIO2_B7_D-PadH25)")
			(pinfunction "GPIO2_B7_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "6185a702-c5c4-47d5-8d2d-f4508fb31267")
		)
		(pad "H26" smd circle
			(at 7.475 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 227 "unconnected-(U1I-GPIO1_D7_U-PadH26)")
			(pinfunction "GPIO1_D7_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "832d6623-6432-4655-819d-ee6f8f679f5b")
		)
		(pad "H27" smd circle
			(at 8.125 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "unconnected-(U1I-GPIO2_A1_U-PadH27)")
			(pinfunction "GPIO2_A1_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "06c96e62-41a9-4065-bf76-0b8e901d51bb")
		)
		(pad "H28" smd circle
			(at 8.775 -4.225)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 248 "unconnected-(U1I-GPIO2_A2_D-PadH28)")
			(pinfunction "GPIO2_A2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "9016fa8e-c9cb-45fd-b8cb-22626d2917d0")
		)
		(pad "J1" smd circle
			(at -8.775 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 244 "unconnected-(U1E-DDR_DQ4_A-PadJ1)")
			(pinfunction "DDR_DQ4_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "8e5be995-a9dc-4bf0-8261-2bd777e8b63a")
		)
		(pad "J2" smd circle
			(at -8.125 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 157 "unconnected-(U1E-DDR_DQ5_A-PadJ2)")
			(pinfunction "DDR_DQ5_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "54e69913-5472-4c1a-98b2-3493043b872a")
		)
		(pad "J3" smd circle
			(at -7.475 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "6aa0ef6b-5dc4-4cc2-a9fe-1a7119bce060")
		)
		(pad "J4" smd circle
			(at -6.825 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 292 "unconnected-(U1E-DDR_DM1_A-PadJ4)")
			(pinfunction "DDR_DM1_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "af2418c1-7df2-4f5e-8cda-7d11b0401096")
		)
		(pad "J5" smd circle
			(at -6.175 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "5d8a0ae9-7654-4188-b88b-20c560a7d7c5")
		)
		(pad "J6" smd circle
			(at -5.525 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 351 "unconnected-(U1E-DDR_DQ13_A-PadJ6)")
			(pinfunction "DDR_DQ13_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "d7f88b11-d9d5-411a-88e8-c8e9c1f3c3c6")
		)
		(pad "J7" smd circle
			(at -4.875 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 215 "unconnected-(U1E-DDR_DQ14_A-PadJ7)")
			(pinfunction "DDR_DQ14_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "7b6b5cba-2f30-481f-9a23-099209f8efa0")
		)
		(pad "J8" smd circle
			(at -4.225 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 250 "unconnected-(U1D-DDR_AVSS-PadJ8)")
			(pinfunction "DDR_AVSS")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "965a5ae6-5ab4-45c3-ab85-3352975fc94a")
		)
		(pad "J9" smd circle
			(at -3.575 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(U1D-DDRPHY_VDDQ-PadH11)")
			(pinfunction "DDRPHY_VDDQ")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "e8fdbaf1-b29e-44df-8791-00482cc7fce5")
		)
		(pad "J11" smd circle
			(at -2.275 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(U1D-DDRPHY_VDDQL-PadJ11)")
			(pinfunction "DDRPHY_VDDQL")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "24b5103b-fa18-4c08-9373-6fc5d40aeb48")
		)
		(pad "J12" smd circle
			(at -1.625 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(U1D-DDRPHY_VDDQL-PadJ11)")
			(pinfunction "DDRPHY_VDDQL")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "4680c476-3ca7-4687-928b-d7647dfd3244")
		)
		(pad "J14" smd circle
			(at -0.325 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(U1D-DDRPHY_VDDQL-PadJ11)")
			(pinfunction "DDRPHY_VDDQL")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "eb090b06-7cec-4056-9b3e-43179b7272a7")
		)
		(pad "J15" smd circle
			(at 0.325 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(U1A-VDD_CPU-PadJ15)")
			(pinfunction "VDD_CPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ed9de184-7ffe-450b-863d-75f75115e39b")
		)
		(pad "J17" smd circle
			(at 1.625 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "3516b4aa-5181-45d2-8071-fa4eb40b14ef")
		)
		(pad "J18" smd circle
			(at 2.275 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "b754c863-d51c-4fb1-aacb-2c578a012eb5")
		)
		(pad "J20" smd circle
			(at 3.575 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "3d627e1a-1a76-4505-a27a-e44354fce7fc")
		)
		(pad "J21" smd circle
			(at 4.225 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 247 "unconnected-(U1J-VCCIO4-PadJ21)")
			(pinfunction "VCCIO4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "900d0bf4-3fa5-4ab8-a705-5e9e1564022d")
		)
		(pad "J22" smd circle
			(at 4.875 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d60c1c23-f061-4f9a-af22-0a3a24724071")
		)
		(pad "J23" smd circle
			(at 5.525 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "unconnected-(U1I-GPIO2_A0_U-PadJ23)")
			(pinfunction "GPIO2_A0_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "1d88ee34-f089-4787-b657-a818e25b49e0")
		)
		(pad "J24" smd circle
			(at 6.175 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 126 "unconnected-(U1I-GPIO1_D6_U-PadJ24)")
			(pinfunction "GPIO1_D6_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "40f191ed-0c6e-4a90-b3c7-c0ec60a97188")
		)
		(pad "J25" smd circle
			(at 6.825 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 133 "unconnected-(U1I-GPIO1_D5_U-PadJ25)")
			(pinfunction "GPIO1_D5_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "4418e468-ac3b-4d50-b28d-9016c60fa202")
		)
		(pad "J26" smd circle
			(at 7.475 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "91d948c9-08b6-49a6-bd6d-0818258d5aed")
		)
		(pad "J27" smd circle
			(at 8.125 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "db635120-d990-448e-aa69-29642d989305")
		)
		(pad "J28" smd circle
			(at 8.775 -3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 240 "unconnected-(U1S-EDP_TX_D0P-PadJ28)")
			(pinfunction "EDP_TX_D0P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "8b4cf45a-3fa0-44ee-b8ca-430f7b0e8b27")
		)
		(pad "K1" smd circle
			(at -8.775 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "eaf87534-38e6-40af-b870-5b6d9c92de05")
		)
		(pad "K2" smd circle
			(at -8.125 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "unconnected-(U1E-DDR_DQ12_A-PadK2)")
			(pinfunction "DDR_DQ12_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "287be62f-33d3-422a-84c5-e6cb4c0d85a3")
		)
		(pad "K10" smd circle
			(at -2.925 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(U1D-DDRPHY_VDDQL-PadJ11)")
			(pinfunction "DDRPHY_VDDQL")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "0a73c8c5-657b-4898-ac9e-98fd5c0df157")
		)
		(pad "K11" smd circle
			(at -2.275 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(U1B-VSS4-PadG17)")
			(pinfunction "VSS4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "5fccc556-8585-47dc-8e3c-1d9b7ed0236f")
		)
		(pad "K12" smd circle
			(at -1.625 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "6a468440-7f4e-4a0c-8b77-3e770dc6adbf")
		)
		(pad "K13" smd circle
			(at -0.975 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "3c3d9563-f966-4271-8e72-bac70e310f39")
		)
		(pad "K14" smd circle
			(at -0.325 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "5268cc61-8f99-45c5-8c1b-39945a24aada")
		)
		(pad "K15" smd circle
			(at 0.325 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(U1A-VDD_CPU-PadJ15)")
			(pinfunction "VDD_CPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "b04f8d5c-8c96-4cae-a9ae-b8dd83272827")
		)
		(pad "K16" smd circle
			(at 0.975 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(U1A-VDD_CPU-PadJ15)")
			(pinfunction "VDD_CPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "be2e9dfe-a81a-498e-8d38-efd7ece29eef")
		)
		(pad "K17" smd circle
			(at 1.625 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(U1A-VDD_CPU-PadJ15)")
			(pinfunction "VDD_CPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "093a8521-d334-483e-a2eb-8593a7f53b89")
		)
		(pad "K18" smd circle
			(at 2.275 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(U1A-VDD_CPU-PadJ15)")
			(pinfunction "VDD_CPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "eefe5176-8f4e-4a4c-a3af-7de2488763ce")
		)
		(pad "K19" smd circle
			(at 2.925 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "11865109-b83c-4a1c-863c-d48f1ebe6f9c")
		)
		(pad "K27" smd circle
			(at 8.125 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 382 "unconnected-(U1S-EDP_TX_D0N-PadK27)")
			(pinfunction "EDP_TX_D0N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "f17c8fb1-8fc2-4abb-8126-5415c88d5374")
		)
		(pad "K28" smd circle
			(at 8.775 -2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 114 "unconnected-(U1S-EDP_TX_D1P-PadK28)")
			(pinfunction "EDP_TX_D1P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "3889faba-db3c-4fee-832c-bb9e69a12e4a")
		)
		(pad "L1" smd circle
			(at -8.775 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 354 "unconnected-(U1E-DDR_DQS1N_A-PadL1)")
			(pinfunction "DDR_DQS1N_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "dafa19c5-ccab-45a7-b1b8-187c9c3e8486")
		)
		(pad "L2" smd circle
			(at -8.125 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 119 "unconnected-(U1E-DDR_DQS1P_A-PadL2)")
			(pinfunction "DDR_DQS1P_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "3b320ee1-1af1-4f89-b7f1-c5fa8e61971d")
		)
		(pad "L3" smd circle
			(at -7.475 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "0e48d2bb-6099-46b7-999f-61dd77a01491")
		)
		(pad "L4" smd circle
			(at -6.825 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 277 "unconnected-(U1E-DDR_DQ15_A-PadL4)")
			(pinfunction "DDR_DQ15_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "abb7fbf2-7230-4371-9ce4-3e4fcea58ddc")
		)
		(pad "L5" smd circle
			(at -6.175 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "7750c9ef-2e33-456a-966b-1b5511df485c")
		)
		(pad "L6" smd circle
			(at -5.525 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 146 "unconnected-(U1E-DDR_DQ11_A-PadL6)")
			(pinfunction "DDR_DQ11_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "4d8d90df-491a-4c02-a517-57b7c46ab5f1")
		)
		(pad "L7" smd circle
			(at -4.875 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 326 "unconnected-(U1E-DDR_DQ10_A-PadL7)")
			(pinfunction "DDR_DQ10_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c1fa8547-41b7-4de9-9f2d-09951b7932ba")
		)
		(pad "L8" smd circle
			(at -4.225 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "725d373a-defe-4720-a339-d92653eab326")
		)
		(pad "L9" smd circle
			(at -3.575 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(U1D-DDRPHY_VDDQ-PadH11)")
			(pinfunction "DDRPHY_VDDQ")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "577d575e-ae81-4a54-afe2-a36e5e3f70d8")
		)
		(pad "L10" smd circle
			(at -2.925 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(U1D-DDRPHY_VDDQL-PadJ11)")
			(pinfunction "DDRPHY_VDDQL")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "a9d412a1-bfca-41a8-9ced-f403f79b40d2")
		)
		(pad "L11" smd circle
			(at -2.275 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d25a4f5c-031e-4bd7-a212-7ffac818ffbb")
		)
		(pad "L12" smd circle
			(at -1.625 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(U1A-VDD_LOGIC-PadL12)")
			(pinfunction "VDD_LOGIC")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "5c5afc5a-e50a-4548-8c14-06e0f55cacd9")
		)
		(pad "L13" smd circle
			(at -0.975 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "0cf07ad9-8247-4190-9a33-93507fadc549")
		)
		(pad "L14" smd circle
			(at -0.325 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "3aa78a2a-231e-4f81-a60a-cd393fbf02ee")
		)
		(pad "L15" smd circle
			(at 0.325 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(U1A-VDD_CPU-PadJ15)")
			(pinfunction "VDD_CPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "51ce3d3b-d50d-46b4-8edd-969877bfddfe")
		)
		(pad "L16" smd circle
			(at 0.975 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(U1A-VDD_CPU-PadJ15)")
			(pinfunction "VDD_CPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ccea487b-6c02-48d3-9af5-ed41937cb63e")
		)
		(pad "L17" smd circle
			(at 1.625 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(U1A-VDD_CPU-PadJ15)")
			(pinfunction "VDD_CPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "318ff668-6117-4a91-bde0-ed84a0c2d7d4")
		)
		(pad "L18" smd circle
			(at 2.275 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(U1A-VDD_CPU-PadJ15)")
			(pinfunction "VDD_CPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "cd71245e-5ea6-437f-8b9d-eed1bc5734b2")
		)
		(pad "L19" smd circle
			(at 2.925 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "6e39f3c4-3fb7-4593-8892-6c73c2ddda83")
		)
		(pad "L20" smd circle
			(at 3.575 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "e0254564-bed7-4a76-ad19-79e2f33d172d")
		)
		(pad "L21" smd circle
			(at 4.225 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "91592cf2-6b32-4a46-b8c6-218a0088ac83")
		)
		(pad "L22" smd circle
			(at 4.875 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 147 "unconnected-(U1I-VCCIO3-PadL22)")
			(pinfunction "VCCIO3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "4e76cbb8-645d-494d-a026-cda3f0d1de2b")
		)
		(pad "L23" smd circle
			(at 5.525 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 297 "unconnected-(U1T-USB3_OTG0_ID-PadL23)")
			(pinfunction "USB3_OTG0_ID")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "b1ddab24-6ff4-4518-9f8b-7356a7355402")
		)
		(pad "L24" smd circle
			(at 6.175 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "2d2e8cfd-1ed4-45f3-acce-566dc523de18")
		)
		(pad "L25" smd circle
			(at 6.825 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 325 "unconnected-(U1S-EDP_TX_AUXP-PadL25)")
			(pinfunction "EDP_TX_AUXP")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c1e59e64-dc90-4ccf-8978-7c26bf1af36b")
		)
		(pad "L26" smd circle
			(at 7.475 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "cfc64070-76fe-47d3-a1e2-5cabe9efc002")
		)
		(pad "L27" smd circle
			(at 8.125 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 123 "unconnected-(U1S-EDP_TX_D1N-PadL27)")
			(pinfunction "EDP_TX_D1N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "3fde83c5-6c40-41db-ae26-02af946e02b1")
		)
		(pad "L28" smd circle
			(at 8.775 -2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 374 "unconnected-(U1S-EDP_TX_D2P-PadL28)")
			(pinfunction "EDP_TX_D2P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "ec6b3439-fbae-4a74-a1c5-a93dc9683f8b")
		)
		(pad "M1" smd circle
			(at -8.775 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 221 "unconnected-(U1E-DDR_DQ8_A-PadM1)")
			(pinfunction "DDR_DQ8_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "7f3ca8d9-48a0-41f2-8c49-d0f81bf1071b")
		)
		(pad "M2" smd circle
			(at -8.125 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "8fd28577-ba33-47c8-b30a-c528e4cb5482")
		)
		(pad "M3" smd circle
			(at -7.475 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(U1B-VSS5-PadK12)")
			(pinfunction "VSS5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "6065abeb-2414-4f00-8134-c85273f01dcc")
		)
		(pad "M4" smd circle
			(at -6.825 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 175 "unconnected-(U1E-DDR_ECC_DQ1-PadM4)")
			(pinfunction "DDR_ECC_DQ1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "61fbdbbd-fc43-4eac-8f17-723ecad8c49d")
		)
		(pad "M5" smd circle
			(at -6.175 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 370 "unconnected-(U1E-DDR_ECC_DQ2-PadM5)")
			(pinfunction "DDR_ECC_DQ2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ebb59c88-6e0f-47a0-bbe1-29327b58ffcc")
		)
		(pad "M6" smd circle
			(at -5.525 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "8a230d07-5732-4fac-b0e2-9012ce384cd5")
		)
		(pad "M7" smd circle
			(at -4.875 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "unconnected-(U1E-DDR_ECC_DQ4-PadM7)")
			(pinfunction "DDR_ECC_DQ4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "1ed16d0d-e193-4421-886a-6daca4ec6fda")
		)
		(pad "M8" smd circle
			(at -4.225 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "bc8ea91e-c2e9-4951-934d-4d0e2ae2855f")
		)
		(pad "M9" smd circle
			(at -3.575 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(U1D-DDRPHY_VDDQ-PadH11)")
			(pinfunction "DDRPHY_VDDQ")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "88fa7e10-a70c-4ef4-a4df-6ba610a6d90c")
		)
		(pad "M10" smd circle
			(at -2.925 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(U1D-DDRPHY_VDDQL-PadJ11)")
			(pinfunction "DDRPHY_VDDQL")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "b4010b1e-814c-48aa-99e4-b1f0a708a613")
		)
		(pad "M11" smd circle
			(at -2.275 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "f5e3f93c-0422-48cd-8e9e-5f2c15d7eb65")
		)
		(pad "M12" smd circle
			(at -1.625 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(U1A-VDD_LOGIC-PadL12)")
			(pinfunction "VDD_LOGIC")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d81644fc-14fa-428f-9cea-49364620af76")
		)
		(pad "M13" smd circle
			(at -0.975 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "f7aff32c-d70f-4851-872c-195fea06902c")
		)
		(pad "M14" smd circle
			(at -0.325 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "b5d34f61-7b3d-4487-9d60-0ea586802a9b")
		)
		(pad "M15" smd circle
			(at 0.325 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 381 "unconnected-(U1A-VDD_CPU_COM-PadM15)")
			(pinfunction "VDD_CPU_COM")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "f106cd79-3868-4ec6-b43f-96d339e8a9f4")
		)
		(pad "M16" smd circle
			(at 0.975 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "9db96f11-c5fc-4614-b3ce-a3f4a2993d39")
		)
		(pad "M17" smd circle
			(at 1.625 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(U1A-VDD_CPU-PadJ15)")
			(pinfunction "VDD_CPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "fba77870-5e67-4eee-a209-79b94de4b0e1")
		)
		(pad "M18" smd circle
			(at 2.275 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "438014e4-5b18-4d4c-a919-2cbf19051ff2")
		)
		(pad "M19" smd circle
			(at 2.925 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(U1A-VDD_NPU-PadM19)")
			(pinfunction "VDD_NPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "10d8d7c9-d7ab-476d-8141-517e52d18da2")
		)
		(pad "M20" smd circle
			(at 3.575 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 153 "unconnected-(U1S-EDP_TX_AVDD_0V9-PadM20)")
			(pinfunction "EDP_TX_AVDD_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "523aa7e1-0ee1-4cb9-a33a-ee9c78734e5c")
		)
		(pad "M21" smd circle
			(at 4.225 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "9abecadb-b293-4020-8b14-011ac75ff7ae")
		)
		(pad "M22" smd circle
			(at 4.875 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 314 "unconnected-(U1S-EDP_TX_AVDD_1V8-PadM22)")
			(pinfunction "EDP_TX_AVDD_1V8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "bd0ba748-8714-4267-bb69-508d5d582ca4")
		)
		(pad "M23" smd circle
			(at 5.525 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "unconnected-(U1T-USB3_AVDD_3V3-PadM23)")
			(pinfunction "USB3_AVDD_3V3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "1335f559-1967-4d1f-b795-c0347f99d744")
		)
		(pad "M24" smd circle
			(at 6.175 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 388 "unconnected-(U1T-USB3_OTG0_VBUSDET-PadM24)")
			(pinfunction "USB3_OTG0_VBUSDET")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "f931c97a-d2f5-4fb2-a5f1-0a16b9174f59")
		)
		(pad "M25" smd circle
			(at 6.825 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 137 "unconnected-(U1S-EDP_TX_AUXN-PadM25)")
			(pinfunction "EDP_TX_AUXN")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "45f4db78-a9c2-42c9-b62b-df2d9598424f")
		)
		(pad "M26" smd circle
			(at 7.475 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "b7ca1ccb-4082-4880-9496-14e218f1ff33")
		)
		(pad "M27" smd circle
			(at 8.125 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(U1S-EDP_TX_D2N-PadM27)")
			(pinfunction "EDP_TX_D2N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "080e3d17-71e3-4132-8621-ff686683b9d2")
		)
		(pad "M28" smd circle
			(at 8.775 -1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 117 "unconnected-(U1S-EDP_TX_D3P-PadM28)")
			(pinfunction "EDP_TX_D3P")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "39eba1f7-63c9-402b-973a-a3b8d55d86bc")
		)
		(pad "N1" smd circle
			(at -8.775 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "b2530e55-976a-4ff7-81a5-cab49d32b524")
		)
		(pad "N2" smd circle
			(at -8.125 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "unconnected-(U1E-DDR_DQ9_A-PadN2)")
			(pinfunction "DDR_DQ9_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "21aa84ae-c9b2-4602-b51a-bf3fdbfdaf53")
		)
		(pad "N10" smd circle
			(at -2.925 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 255 "unconnected-(U1F-SYSPLL_AVDD_1V8-PadN10)")
			(pinfunction "SYSPLL_AVDD_1V8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "9cb94303-c897-4d41-a4b5-3f1018d0e4a1")
		)
		(pad "N11" smd circle
			(at -2.275 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 189 "unconnected-(U1F-SYSPLL_AVSS-PadN11)")
			(pinfunction "SYSPLL_AVSS")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "6c26b3cb-7d67-424c-a764-b60a3e05edc9")
		)
		(pad "N12" smd circle
			(at -1.625 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "1ec96a8f-c866-45b7-bf68-f5219a44314f")
		)
		(pad "N13" smd circle
			(at -0.975 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(U1A-VDD_LOGIC-PadL12)")
			(pinfunction "VDD_LOGIC")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "492eb6e6-ac34-4636-9e51-df23f38d06f3")
		)
		(pad "N14" smd circle
			(at -0.325 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "beada0cb-e870-4caf-8103-c32f46f2c1d2")
		)
		(pad "N15" smd circle
			(at 0.325 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "95596f60-7cab-4d4c-8636-673581860654")
		)
		(pad "N16" smd circle
			(at 0.975 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(U1A-VDD_LOGIC-PadL12)")
			(pinfunction "VDD_LOGIC")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "554eb34f-8083-4288-b811-68d608bf6189")
		)
		(pad "N17" smd circle
			(at 1.625 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d18a2801-d555-47e5-8104-edb6fa45783d")
		)
		(pad "N18" smd circle
			(at 2.275 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c8b76683-f851-4bae-afde-f54e78144f9e")
		)
		(pad "N19" smd circle
			(at 2.925 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(U1A-VDD_NPU-PadM19)")
			(pinfunction "VDD_NPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "bd440f4e-49a3-4d57-8c2d-aec9c7b7c692")
		)
		(pad "N27" smd circle
			(at 8.125 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "unconnected-(U1S-EDP_TX_D3N-PadN27)")
			(pinfunction "EDP_TX_D3N")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "25d508bb-5dc0-48a4-b8c1-254f08e699d4")
		)
		(pad "N28" smd circle
			(at 8.775 -0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c8ab6b47-d5bd-42f6-96d5-e8f184c81d34")
		)
		(pad "P1" smd circle
			(at -8.775 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 229 "unconnected-(U1E-DDR_ECC_DQS_N-PadP1)")
			(pinfunction "DDR_ECC_DQS_N")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "8521afd9-0e64-4008-a288-c839749219ec")
		)
		(pad "P2" smd circle
			(at -8.125 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 246 "unconnected-(U1E-DDR_ECC_DQS_P-PadP2)")
			(pinfunction "DDR_ECC_DQS_P")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "8fcbae7f-3bc3-4f89-b493-f6e07c147942")
		)
		(pad "P3" smd circle
			(at -7.475 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "998095c8-e3f4-4034-9730-f5600877ce88")
		)
		(pad "P4" smd circle
			(at -6.825 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 383 "unconnected-(U1E-DDR_ECC_DQ6-PadP4)")
			(pinfunction "DDR_ECC_DQ6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "f25a0495-56f3-440a-b364-4465b4414568")
		)
		(pad "P5" smd circle
			(at -6.175 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 361 "unconnected-(U1E-DDR_ECC_DQ0-PadP5)")
			(pinfunction "DDR_ECC_DQ0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "e371ee56-f313-4f0f-ae8b-69d0e590f92f")
		)
		(pad "P6" smd circle
			(at -5.525 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(U1B-VSS6-PadM11)")
			(pinfunction "VSS6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "24f0df4d-47fb-4720-a0f1-0af0860e4c95")
		)
		(pad "P7" smd circle
			(at -4.875 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 128 "unconnected-(U1E-DDR_ECC_DM-PadP7)")
			(pinfunction "DDR_ECC_DM")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "41c975da-7286-40d8-87f4-48107c45589b")
		)
		(pad "P8" smd circle
			(at -4.225 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 342 "unconnected-(U1E-DDR_VREFOUT-PadP8)")
			(pinfunction "DDR_VREFOUT")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "cd16d324-f0ba-4518-b56f-192ddd0a1356")
		)
		(pad "P9" smd circle
			(at -3.575 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 352 "unconnected-(U1U-USB2_AVDD_1V8-PadP9)")
			(pinfunction "USB2_AVDD_1V8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d8fdf5d9-3f57-4969-b3da-30d17a18c74e")
		)
		(pad "P10" smd circle
			(at -2.925 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "unconnected-(U1U-USB2_AVDD_3V3-PadP10)")
			(pinfunction "USB2_AVDD_3V3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "1a813613-b759-4aa3-8588-9367acf0cbcc")
		)
		(pad "P11" smd circle
			(at -2.275 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 200 "unconnected-(U1F-SYSPLL_AVDD_0V9-PadP11)")
			(pinfunction "SYSPLL_AVDD_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "73cdb1d1-c478-4d08-a9ab-3e8bb68f6e35")
		)
		(pad "P12" smd circle
			(at -1.625 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "23488f4d-f147-4a3c-84db-5635b68684aa")
		)
		(pad "P13" smd circle
			(at -0.975 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(U1A-VDD_LOGIC-PadL12)")
			(pinfunction "VDD_LOGIC")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "26a77132-bc8f-4aec-9ed0-881bf046a645")
		)
		(pad "P14" smd circle
			(at -0.325 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "203b0b3f-cdbd-4e8a-8dea-cc2afd55926f")
		)
		(pad "P15" smd circle
			(at 0.325 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "42f3b63f-f8e9-4001-bcfb-8d02f19d18d3")
		)
		(pad "P16" smd circle
			(at 0.975 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(U1A-VDD_LOGIC-PadL12)")
			(pinfunction "VDD_LOGIC")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "fcbcbdbe-9953-477f-a848-4e600ad79748")
		)
		(pad "P17" smd circle
			(at 1.625 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "3fed2eac-dfa1-47f4-b687-1c12e02a5b5f")
		)
		(pad "P18" smd circle
			(at 2.275 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(U1A-VDD_NPU-PadM19)")
			(pinfunction "VDD_NPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "960bdf80-cfff-443f-868f-e03cef33c4fd")
		)
		(pad "P19" smd circle
			(at 2.925 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(U1A-VDD_NPU-PadM19)")
			(pinfunction "VDD_NPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ba720295-02e9-4581-8009-bc58fe793ed8")
		)
		(pad "P20" smd circle
			(at 3.575 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(U1A-VDD_NPU-PadM19)")
			(pinfunction "VDD_NPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "6d89173e-1177-4690-81e3-6c0417cdba45")
		)
		(pad "P21" smd circle
			(at 4.225 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "7464a540-0949-4fa1-bda2-70f9a5790f41")
		)
		(pad "P22" smd circle
			(at 4.875 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "unconnected-(U1T-USB3_AVDD_0V9-PadP22)")
			(pinfunction "USB3_AVDD_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "1201cda0-7944-4cf4-95dc-e645154c80cc")
		)
		(pad "P23" smd circle
			(at 5.525 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "unconnected-(U1T-USB3_AVDD_1V8-PadP23)")
			(pinfunction "USB3_AVDD_1V8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "1ffff19c-627e-4510-9843-e1df80f6350a")
		)
		(pad "P24" smd circle
			(at 6.175 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "unconnected-(U1T-USB3_HOST1_DP-PadP24)")
			(pinfunction "USB3_HOST1_DP")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "283b39dc-7ff3-45f3-8b16-5799079930b9")
		)
		(pad "P25" smd circle
			(at 6.825 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 390 "unconnected-(U1T-USB3_HOST1_DM-PadP25)")
			(pinfunction "USB3_HOST1_DM")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "f99b56d4-41d9-45fd-93b1-198b5f859911")
		)
		(pad "P26" smd circle
			(at 7.475 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d9548780-7851-40a9-9223-f55e8b7f6bfb")
		)
		(pad "P27" smd circle
			(at 8.125 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 253 "unconnected-(U1T-USB3_OTG0_DP-PadP27)")
			(pinfunction "USB3_OTG0_DP")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "9993f850-3f48-4355-b5d1-64ceeb52a622")
		)
		(pad "P28" smd circle
			(at 8.775 -0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 219 "unconnected-(U1T-USB3_OTG0_DM-PadP28)")
			(pinfunction "USB3_OTG0_DM")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "7ce01afb-4c4d-4780-9fd0-97ec31144820")
		)
		(pad "R1" smd circle
			(at -8.775 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "unconnected-(U1U-USB2_HOST2_DM-PadR1)")
			(pinfunction "USB2_HOST2_DM")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "0b10f292-0c4a-412c-acf9-2edd3838b44c")
		)
		(pad "R2" smd circle
			(at -8.125 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "unconnected-(U1U-USB2_HOST2_DP-PadR2)")
			(pinfunction "USB2_HOST2_DP")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "1e148ba9-2f9d-4296-8811-d205a49a3dc0")
		)
		(pad "R3" smd circle
			(at -7.475 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "cbf9e247-0be6-474f-a798-dc4a67b83389")
		)
		(pad "R4" smd circle
			(at -6.825 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 329 "unconnected-(U1E-DDR_ECC_DQ7-PadR4)")
			(pinfunction "DDR_ECC_DQ7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c3b23728-d9d1-428f-8e54-d71fd8305761")
		)
		(pad "R5" smd circle
			(at -6.175 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 204 "unconnected-(U1E-DDR_ECC_DQ3-PadR5)")
			(pinfunction "DDR_ECC_DQ3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "762d23e7-1121-4b5b-9994-491d0b41ee49")
		)
		(pad "R6" smd circle
			(at -5.525 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "20dbe00a-5c23-4e62-83d0-6d55d9437bac")
		)
		(pad "R7" smd circle
			(at -4.875 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 149 "unconnected-(U1E-DDR_ECC_DQ5-PadR7)")
			(pinfunction "DDR_ECC_DQ5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "50945b39-c62f-477f-9f1b-584f1ef66e08")
		)
		(pad "R8" smd circle
			(at -4.225 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 393 "unconnected-(U1U-USB2_AVDD_0V9-PadR8)")
			(pinfunction "USB2_AVDD_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "fad231f7-2729-4bcf-8f4e-f08d3ec004ec")
		)
		(pad "R9" smd circle
			(at -3.575 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "Net-(U1L-VCCIO6-PadR9)")
			(pinfunction "VCCIO6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "0d5c298b-51eb-4f30-ab3c-e2c19e1d10c6")
		)
		(pad "R10" smd circle
			(at -2.925 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "a1ba4868-68ca-4c2b-a3aa-2376191cbfdb")
		)
		(pad "R11" smd circle
			(at -2.275 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "da655c5e-8ceb-402b-bb1f-8554d805a811")
		)
		(pad "R12" smd circle
			(at -1.625 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(U1A-VDD_LOGIC-PadL12)")
			(pinfunction "VDD_LOGIC")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c09d000e-b753-458f-b7bd-41c85f246954")
		)
		(pad "R13" smd circle
			(at -0.975 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "Net-(U1A-VDD_GPU-PadR13)")
			(pinfunction "VDD_GPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d450aeeb-9a9f-4664-bec4-17f135b512d7")
		)
		(pad "R14" smd circle
			(at -0.325 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "187e2d71-dcb8-4b1c-88c8-7a0ad1f923e6")
		)
		(pad "R15" smd circle
			(at 0.325 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "15d4cb35-3dc3-4732-9c7f-00c964ed9989")
		)
		(pad "R16" smd circle
			(at 0.975 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(U1A-VDD_LOGIC-PadL12)")
			(pinfunction "VDD_LOGIC")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "4d406f5d-eacb-4787-befd-722cb37f5346")
		)
		(pad "R17" smd circle
			(at 1.625 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "e8ec78e8-a004-499b-b36f-c65593e88a9a")
		)
		(pad "R18" smd circle
			(at 2.275 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "000372db-985a-42c8-86c5-a8c162fe515e")
		)
		(pad "R19" smd circle
			(at 2.925 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "7ec1788e-e4bc-4979-8dad-6dab04282581")
		)
		(pad "R20" smd circle
			(at 3.575 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "Net-(U1T-MULTI_PHY_AVDD_0V9-PadR20)")
			(pinfunction "MULTI_PHY_AVDD_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "487024da-cfdb-4569-84a6-4a8f8366060f")
		)
		(pad "R21" smd circle
			(at 4.225 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "Net-(U1T-MULTI_PHY_AVDD_0V9-PadR20)")
			(pinfunction "MULTI_PHY_AVDD_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "1894d03f-68da-4e6a-92d4-e711557133dc")
		)
		(pad "R22" smd circle
			(at 4.875 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 206 "unconnected-(U1T-MULTI_PHY_AVDD_1V8-PadR22)")
			(pinfunction "MULTI_PHY_AVDD_1V8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "76de80c1-7675-4b33-9508-1941cc59e4e1")
		)
		(pad "R23" smd circle
			(at 5.525 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "9f3c7322-612a-494a-bfd8-7b1485f65bc6")
		)
		(pad "R24" smd circle
			(at 6.175 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 171 "unconnected-(U1T-MULTI_PHY0_REFCLKP-PadR24)")
			(pinfunction "MULTI_PHY0_REFCLKP")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "60243817-b846-4be4-b4c8-6781d31b9048")
		)
		(pad "R25" smd circle
			(at 6.825 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 228 "unconnected-(U1T-MULTI_PHY0_REFCLKN-PadR25)")
			(pinfunction "MULTI_PHY0_REFCLKN")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "84b538b3-1582-4597-8c9e-b3eeaf373097")
		)
		(pad "R26" smd circle
			(at 7.475 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "20c19512-27ed-4ee7-9c66-3c71edf85ccb")
		)
		(pad "R27" smd circle
			(at 8.125 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 141 "unconnected-(U1T-USB3_OTG0_SSRXN{slash}SATA0_RXN-PadR27)")
			(pinfunction "USB3_OTG0_SSRXN/SATA0_RXN")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "48f6daa4-4f1c-4ff9-b7ad-b01fdd358b69")
		)
		(pad "R28" smd circle
			(at 8.775 0.325)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 304 "unconnected-(U1T-USB3_OTG0_SSRXP{slash}SATA0_RXP-PadR28)")
			(pinfunction "USB3_OTG0_SSRXP/SATA0_RXP")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "b4ca5947-ea20-4281-8411-d30cbab824e1")
		)
		(pad "T1" smd circle
			(at -8.775 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "unconnected-(U1U-USB2_HOST3_DM-PadT1)")
			(pinfunction "USB2_HOST3_DM")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "2c6a6420-b680-4d42-ba27-7f6fd5918614")
		)
		(pad "T2" smd circle
			(at -8.125 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 193 "unconnected-(U1U-USB2_HOST3_DP-PadT2)")
			(pinfunction "USB2_HOST3_DP")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "6ff5d1d8-28b4-4be2-9911-8b7ed59ca65b")
		)
		(pad "T10" smd circle
			(at -2.925 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ea5d9c8a-2c9d-4077-9524-20cd6adf93cc")
		)
		(pad "T11" smd circle
			(at -2.275 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U1C-VSS7-PadP12)")
			(pinfunction "VSS7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "9512140a-aa0e-43c3-817a-6dc4fcfcc066")
		)
		(pad "T12" smd circle
			(at -1.625 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(U1A-VDD_LOGIC-PadL12)")
			(pinfunction "VDD_LOGIC")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ce5738c2-b055-4372-bdf8-5be385c1af93")
		)
		(pad "T13" smd circle
			(at -0.975 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "Net-(U1A-VDD_GPU-PadR13)")
			(pinfunction "VDD_GPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "b3327232-3541-4c55-9ee2-24bbe8f2be7f")
		)
		(pad "T14" smd circle
			(at -0.325 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "028e30b1-412e-4377-8798-fc2ef2b171a9")
		)
		(pad "T15" smd circle
			(at 0.325 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "6128fa86-d4eb-478b-88a8-759db7865a6f")
		)
		(pad "T16" smd circle
			(at 0.975 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(U1A-VDD_LOGIC-PadL12)")
			(pinfunction "VDD_LOGIC")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "7b0dbadd-36ba-4658-816a-5c8ca1857eb4")
		)
		(pad "T17" smd circle
			(at 1.625 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "cb7724c8-3270-43b8-9b09-a7c572241518")
		)
		(pad "T18" smd circle
			(at 2.275 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d8488c01-5a27-464b-afc0-d90112aaa991")
		)
		(pad "T19" smd circle
			(at 2.925 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "806cf41c-8088-4770-beed-ad2f46de24c1")
		)
		(pad "T27" smd circle
			(at 8.125 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "unconnected-(U1T-USB3_OTG0_SSTXN{slash}SATA0_TXN-PadT27)")
			(pinfunction "USB3_OTG0_SSTXN/SATA0_TXN")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "2942eef2-605f-4f7c-bc54-fbee8dc0ee12")
		)
		(pad "T28" smd circle
			(at 8.775 0.975)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 259 "unconnected-(U1T-USB3_OTG0_SSTXP{slash}SATA0_TXP-PadT28)")
			(pinfunction "USB3_OTG0_SSTXP/SATA0_TXP")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "9f88848f-41b9-44dc-9deb-c2e57d1e128a")
		)
		(pad "U1" smd circle
			(at -8.775 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "be8b72d7-a555-4463-a185-80dbcf08d24b")
		)
		(pad "U2" smd circle
			(at -8.125 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 241 "unconnected-(U1L-GPIO4_C1_D-PadU2)")
			(pinfunction "GPIO4_C1_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "8c13a586-2628-4b24-99a2-29af2cecf140")
		)
		(pad "U3" smd circle
			(at -7.475 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 355 "unconnected-(U1L-GPIO4_C0_D-PadU3)")
			(pinfunction "GPIO4_C0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "db271840-5e1c-40ce-9349-906cb1d4a1fb")
		)
		(pad "U4" smd circle
			(at -6.825 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 164 "unconnected-(U1L-GPIO4_B7_D-PadU4)")
			(pinfunction "GPIO4_B7_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "5dd0af25-2769-419a-8140-2c6e76102773")
		)
		(pad "U5" smd circle
			(at -6.175 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 152 "unconnected-(U1L-GPIO4_B6_D-PadU5)")
			(pinfunction "GPIO4_B6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "5213dc98-8f28-44be-93a4-c256fc6975c1")
		)
		(pad "U6" smd circle
			(at -5.525 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ebb91bcd-0f0e-4975-9789-427aae9e49ee")
		)
		(pad "U7" smd circle
			(at -4.875 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "dfc81250-a93c-40e9-a8cc-61a93726f329")
		)
		(pad "U8" smd circle
			(at -4.225 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ab7808c4-8dfb-4896-88bb-c476e5597b3f")
		)
		(pad "U9" smd circle
			(at -3.575 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "Net-(U1L-VCCIO6-PadR9)")
			(pinfunction "VCCIO6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "432bcd75-150a-469a-82e8-02a8bc9abd9c")
		)
		(pad "U10" smd circle
			(at -2.925 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "91c69507-6672-439f-8a79-66872b892123")
		)
		(pad "U11" smd circle
			(at -2.275 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "Net-(U1A-VDD_GPU-PadR13)")
			(pinfunction "VDD_GPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "f296e1bf-3e11-42bb-81cd-6ffa0240fe7b")
		)
		(pad "U12" smd circle
			(at -1.625 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "Net-(U1A-VDD_GPU-PadR13)")
			(pinfunction "VDD_GPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "20294297-4bde-4997-b7c7-b6caefd68fc6")
		)
		(pad "U13" smd circle
			(at -0.975 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "Net-(U1A-VDD_GPU-PadR13)")
			(pinfunction "VDD_GPU")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ed74aaf9-0d4d-4915-a2e4-1ba3be4cd24f")
		)
		(pad "U14" smd circle
			(at -0.325 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "7b91fb31-518e-415e-907e-3befa527f38b")
		)
		(pad "U15" smd circle
			(at 0.325 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "7b173211-d02e-48d4-a85e-8b1cea4cc5e4")
		)
		(pad "U16" smd circle
			(at 0.975 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "f4dfa63f-13c3-4e46-ad7b-37322b9622fc")
		)
		(pad "U17" smd circle
			(at 1.625 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "1f7a6b17-197d-442d-9563-5509eb084be0")
		)
		(pad "U18" smd circle
			(at 2.275 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1C-VSS8-PadT14)")
			(pinfunction "VSS8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "f1030542-366c-4e77-b46a-bef7e680849f")
		)
		(pad "U19" smd circle
			(at 2.925 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 125 "unconnected-(U1V-PCIE30_RESREF-PadU19)")
			(pinfunction "PCIE30_RESREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(uuid "40efe53b-3727-4eb5-8fa1-9fdabc3f642c")
		)
		(pad "U20" smd circle
			(at 3.575 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 150 "Net-(U1V-PCIE30_AVDD_0V9-PadU20)")
			(pinfunction "PCIE30_AVDD_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "50b5f2ba-050f-4973-9e73-1baed2ddeefe")
		)
		(pad "U21" smd circle
			(at 4.225 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 150 "Net-(U1V-PCIE30_AVDD_0V9-PadU20)")
			(pinfunction "PCIE30_AVDD_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "8ad2b4ab-48a6-44ae-adb8-c90dc676ae98")
		)
		(pad "U22" smd circle
			(at 4.875 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 212 "unconnected-(U1V-PCIE30_AVDD_1V8-PadU22)")
			(pinfunction "PCIE30_AVDD_1V8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "79fe8f59-e8c6-44da-8441-a2561ea3f583")
		)
		(pad "U23" smd circle
			(at 5.525 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "490320a3-0dd4-4940-9990-80b8d3ee4290")
		)
		(pad "U24" smd circle
			(at 6.175 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "unconnected-(U1T-MULTI_PHY1_REFCLKN-PadU24)")
			(pinfunction "MULTI_PHY1_REFCLKN")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "49fdc615-3683-4b5c-95cf-ae9512cc554b")
		)
		(pad "U25" smd circle
			(at 6.825 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 166 "unconnected-(U1T-MULTI_PHY1_REFCLKP-PadU25)")
			(pinfunction "MULTI_PHY1_REFCLKP")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "5e457160-456c-4f7e-a16e-167604eabe4c")
		)
		(pad "U26" smd circle
			(at 7.475 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "8a834a97-672f-4b8f-ae69-ac47e0a3beeb")
		)
		(pad "U27" smd circle
			(at 8.125 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 167 "unconnected-(U1T-USB3_HOST1_SSRXN{slash}SATA1_RXN{slash}QSGMII_RXN_M0-PadU27)")
			(pinfunction "USB3_HOST1_SSRXN/SATA1_RXN/QSGMII_RXN_M0")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "5f297dde-7ce6-436e-a432-8ead70686910")
		)
		(pad "U28" smd circle
			(at 8.775 1.625)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 313 "unconnected-(U1T-USB3_HOST1_SSRXP{slash}SATA1_RXP{slash}QSGMII_RXP_M0-PadU28)")
			(pinfunction "USB3_HOST1_SSRXP/SATA1_RXP/QSGMII_RXP_M0")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "bca765c6-9fb2-41c5-a46c-461ecde164df")
		)
		(pad "V1" smd circle
			(at -8.775 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 307 "unconnected-(U1L-GPIO4_B3_D-PadV1)")
			(pinfunction "GPIO4_B3_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "b86d8d77-db28-4a57-94b9-aca9b5e03cbe")
		)
		(pad "V2" smd circle
			(at -8.125 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 376 "unconnected-(U1L-GPIO4_B1_D-PadV2)")
			(pinfunction "GPIO4_B1_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ef914e8d-0ce6-44de-8e98-4cf43e378877")
		)
		(pad "V3" smd circle
			(at -7.475 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "8943701f-44a2-4bf1-92f0-b69d9c105e2d")
		)
		(pad "V4" smd circle
			(at -6.825 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "unconnected-(U1L-GPIO4_B2_D-PadV4)")
			(pinfunction "GPIO4_B2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "0a6c7668-fe57-48f2-bdfb-af7642fc41ad")
		)
		(pad "V5" smd circle
			(at -6.175 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "unconnected-(U1L-GPIO4_B5_D-PadV5)")
			(pinfunction "GPIO4_B5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "1f367579-0ea5-4219-bf2b-4dc9a61ec457")
		)
		(pad "V6" smd circle
			(at -5.525 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 273 "unconnected-(U1L-GPIO4_B4_D-PadV6)")
			(pinfunction "GPIO4_B4_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "a9f281de-3a61-409b-907c-573c68e53910")
		)
		(pad "V7" smd circle
			(at -4.875 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 190 "unconnected-(U1L-GPIO4_B0_D-PadV7)")
			(pinfunction "GPIO4_B0_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "6e257b70-d3fa-42b7-a280-a764af8b3359")
		)
		(pad "V8" smd circle
			(at -4.225 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "594219ed-8c2e-47ff-b59e-f7ef3965b76c")
		)
		(pad "V9" smd circle
			(at -3.575 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "5e6907da-2e39-4b68-85d7-ecedc118dfd9")
		)
		(pad "V10" smd circle
			(at -2.925 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 263 "Net-(U1K-VCCIO5-PadV10)")
			(pinfunction "VCCIO5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d155fb2a-d46c-407a-a744-d244e5e2d175")
		)
		(pad "V11" smd circle
			(at -2.275 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 263 "Net-(U1K-VCCIO5-PadV10)")
			(pinfunction "VCCIO5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "a1f86a23-c003-40d2-ac57-b77a310bc917")
		)
		(pad "V12" smd circle
			(at -1.625 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 176 "unconnected-(U1M-VCCIO7-PadV12)")
			(pinfunction "VCCIO7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "62d04228-98e6-4ac8-99e0-30c99b440c05")
		)
		(pad "V13" smd circle
			(at -0.975 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "18ffe708-e63e-4c7a-9217-8318c12dd278")
		)
		(pad "V14" smd circle
			(at -0.325 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "4cdd1cc3-d75f-4024-ab40-54aa8da07bef")
		)
		(pad "V15" smd circle
			(at 0.325 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "94fe5bd6-c320-4ca3-9ae9-132162d9cd5f")
		)
		(pad "V16" smd circle
			(at 0.975 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(U1A-AVSS1-PadJ27)")
			(pinfunction "AVSS1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "8f87ffb5-10aa-4473-896d-c0c615592837")
		)
		(pad "V17" smd circle
			(at 1.625 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "Net-(U1P-HDMI_TX_AVDD_0V9-PadV17)")
			(pinfunction "HDMI_TX_AVDD_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "2c375598-bfa6-4a83-bb15-82a1f93ec341")
		)
		(pad "V18" smd circle
			(at 2.275 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "Net-(U1P-HDMI_TX_AVDD_0V9-PadV17)")
			(pinfunction "HDMI_TX_AVDD_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c10e2c89-2186-4be0-b231-b90a2c48e502")
		)
		(pad "V19" smd circle
			(at 2.925 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "unconnected-(U1F-PMU_VDD_LOGIC_0V9-PadV19)")
			(pinfunction "PMU_VDD_LOGIC_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "268ed51a-4e49-4fb4-8d42-9d37b705c79c")
		)
		(pad "V20" smd circle
			(at 3.575 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 130 "unconnected-(U1F-PMUPLL_AVSS-PadV20)")
			(pinfunction "PMUPLL_AVSS")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "43547343-e271-402d-9c69-975242c7d18f")
		)
		(pad "V21" smd circle
			(at 4.225 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "unconnected-(U1F-PMUPLL_AVDD_0V9-PadV21)")
			(pinfunction "PMUPLL_AVDD_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "243d0b97-33c1-4ff3-9b1e-5ec5f093b888")
		)
		(pad "V22" smd circle
			(at 4.875 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "b7b5b07a-d93c-42f4-adff-ff43be60fdda")
		)
		(pad "V23" smd circle
			(at 5.525 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "ae49fcca-60a9-486e-bb43-62e882300039")
		)
		(pad "V24" smd circle
			(at 6.175 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 372 "unconnected-(U1T-PCIE20_REFCLKP-PadV24)")
			(pinfunction "PCIE20_REFCLKP")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "ec126f21-6170-4d5d-8c65-10247b4bee34")
		)
		(pad "V25" smd circle
			(at 6.825 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "unconnected-(U1T-PCIE20_REFCLKN-PadV25)")
			(pinfunction "PCIE20_REFCLKN")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "23024d6c-aed0-42e9-ac34-15546d33c0f3")
		)
		(pad "V26" smd circle
			(at 7.475 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "547a4c94-7255-4972-9c58-23c37ba432cf")
		)
		(pad "V27" smd circle
			(at 8.125 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "unconnected-(U1T-USB3_HOST1_SSTXN{slash}SATA1_TXN{slash}QSGMII_TXN_M0-PadV27)")
			(pinfunction "USB3_HOST1_SSTXN/SATA1_TXN/QSGMII_TXN_M0")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "111a7088-3a0a-440c-bacb-7077e356e7af")
		)
		(pad "V28" smd circle
			(at 8.775 2.275)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 220 "unconnected-(U1T-USB3_HOST1_SSTXP{slash}SATA1_TXP{slash}QSGMII_TXP_M0-PadV28)")
			(pinfunction "USB3_HOST1_SSTXP/SATA1_TXP/QSGMII_TXP_M0")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "7eac04cf-a862-458c-9103-e395ddce4074")
		)
		(pad "W1" smd circle
			(at -8.775 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 207 "unconnected-(U1L-GPIO4_A7_D-PadW1)")
			(pinfunction "GPIO4_A7_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "77a9afc0-fcaf-406a-a09e-a0b2289e0681")
		)
		(pad "W2" smd circle
			(at -8.125 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "unconnected-(U1L-GPIO4_A6_D-PadW2)")
			(pinfunction "GPIO4_A6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "1ac6803b-e583-42d2-90c7-35758df6622d")
		)
		(pad "W10" smd circle
			(at -2.925 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d1b93f72-2d54-4aeb-be56-58aa7f17d1da")
		)
		(pad "W11" smd circle
			(at -2.275 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "7afdc5a0-c35c-45ca-b4f1-8e8a80d75789")
		)
		(pad "W12" smd circle
			(at -1.625 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "6cc06a0a-d862-4b1f-9bbd-72076a9e1cf8")
		)
		(pad "W13" smd circle
			(at -0.975 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "08da6b8b-ca76-4b95-8e6c-a7e7182d5461")
		)
		(pad "W14" smd circle
			(at -0.325 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 378 "unconnected-(U1O-MIPI_CSI_RX_AVDD_0V9-PadW14)")
			(pinfunction "MIPI_CSI_RX_AVDD_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "efae80fa-fcba-4cd6-8142-78a3763663d7")
		)
		(pad "W15" smd circle
			(at 0.325 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 182 "unconnected-(U1R-MIPI_DSI_TX1_AVDD_0V9-PadW15)")
			(pinfunction "MIPI_DSI_TX1_AVDD_0V9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "66c9ea9e-35dd-43b1-87dd-ae7336a60579")
		)
		(pad "W16" smd circle
			(at 0.975 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "unconnected-(U1Q-MIPI_DSI_TX0{slash}LVDS_TX0_AVDD_0V9-PadW16)")
			(pinfunction "MIPI_DSI_TX0/LVDS_TX0_AVDD_0V9")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "0f3d3ee8-9a2e-4bad-880f-672ecb1f3371")
		)
		(pad "W17" smd circle
			(at 1.625 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "281d619c-a9cb-4e98-bead-7cddbbc033c8")
		)
		(pad "W18" smd circle
			(at 2.275 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 179 "unconnected-(U1P-HDMI_TX_AVDD_1V8-PadW18)")
			(pinfunction "HDMI_TX_AVDD_1V8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "639f0323-2acd-4a04-ac20-cbcba6a41983")
		)
		(pad "W19" smd circle
			(at 2.925 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 331 "unconnected-(U1F-PMUIO2-PadW19)")
			(pinfunction "PMUIO2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "c5e00d77-8122-4d99-b267-e22927fed3a8")
		)
		(pad "W27" smd circle
			(at 8.125 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "unconnected-(U1T-PCIE20_TXP{slash}SATA2_TXP{slash}QSGMII_TXP_M1-PadW27)")
			(pinfunction "PCIE20_TXP/SATA2_TXP/QSGMII_TXP_M1")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "2898c6be-2e22-4bc9-ad7e-6e2735c8a30c")
		)
		(pad "W28" smd circle
			(at 8.775 2.925)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 379 "unconnected-(U1T-PCIE20_TXN{slash}SATA2_TXN{slash}QSGMII_TXN_M1-PadW28)")
			(pinfunction "PCIE20_TXN/SATA2_TXN/QSGMII_TXN_M1")
			(pintype "output")
			(solder_mask_margin 0.102)
			(uuid "f0256d3d-824e-4f39-93bc-04e3cd4e87f7")
		)
		(pad "Y1" smd circle
			(at -8.775 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "unconnected-(U1L-GPIO4_A5_D-PadY1)")
			(pinfunction "GPIO4_A5_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "20ca7d73-146b-4d46-a884-10f7e8c47311")
		)
		(pad "Y2" smd circle
			(at -8.125 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "unconnected-(U1L-GPIO4_A4_D-PadY2)")
			(pinfunction "GPIO4_A4_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "08bdc511-c139-4086-9a60-830267039ef9")
		)
		(pad "Y3" smd circle
			(at -7.475 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "unconnected-(U1L-GPIO4_A3_D-PadY3)")
			(pinfunction "GPIO4_A3_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "24f61f12-8fc0-4e4d-9f5a-ec2e6c25e73b")
		)
		(pad "Y4" smd circle
			(at -6.825 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 270 "unconnected-(U1L-GPIO4_A2_D-PadY4)")
			(pinfunction "GPIO4_A2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "a82118d2-5991-4c4e-8f3f-bcabc32050ae")
		)
		(pad "Y5" smd circle
			(at -6.175 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 234 "unconnected-(U1L-GPIO3_D7_D-PadY5)")
			(pinfunction "GPIO3_D7_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "880a2d3a-bd1a-4ebd-b0d8-05e6f64173e0")
		)
		(pad "Y6" smd circle
			(at -5.525 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 160 "unconnected-(U1L-GPIO3_D6_D-PadY6)")
			(pinfunction "GPIO3_D6_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "578e39f8-5c03-4d85-8989-778bba29ab74")
		)
		(pad "Y7" smd circle
			(at -4.875 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "unconnected-(U1L-GPIO3_D2_D-PadY7)")
			(pinfunction "GPIO3_D2_D")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "27bf67c4-6ece-4860-b50a-99b27ed3664b")
		)
		(pad "Y8" smd circle
			(at -4.225 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "56805ee9-0ae6-4fa8-9dc2-048794f3ee3b")
		)
		(pad "Y9" smd circle
			(at -3.575 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "5a23f116-85c4-4d95-aaeb-c14dc3e17cb5")
		)
		(pad "Y11" smd circle
			(at -2.275 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "0a3eb910-d3f5-4428-be78-d177d8bd7cc1")
		)
		(pad "Y12" smd circle
			(at -1.625 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1C-VSS9-PadAA23)")
			(pinfunction "VSS9")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "d74c8cef-08eb-4c28-bb7e-541ab58207ad")
		)
		(pad "Y14" smd circle
			(at -0.325 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 239 "unconnected-(U1O-MIPI_CSI_RX_AVDD_1V8-PadY14)")
			(pinfunction "MIPI_CSI_RX_AVDD_1V8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "8abc75b9-9179-4002-9825-8971550afa1b")
		)
		(pad "Y15" smd circle
			(at 0.325 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 320 "unconnected-(U1R-MIPI_DSI_TX1_AVDD_1V8-PadY15)")
			(pinfunction "MIPI_DSI_TX1_AVDD_1V8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "bfab7893-b6d8-4f5d-b2a5-e0cecb0bb618")
		)
		(pad "Y17" smd circle
			(at 1.625 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 394 "unconnected-(U1Q-MIPI_DSI_TX0{slash}LVDS_TX0_AVDD_1V8-PadY17)")
			(pinfunction "MIPI_DSI_TX0/LVDS_TX0_AVDD_1V8")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "fb852bc9-6f2b-420d-acdc-3bb8bf80ee49")
		)
		(pad "Y18" smd circle
			(at 2.275 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "21369de9-ff6a-41b1-a7de-132220f7d89e")
		)
		(pad "Y20" smd circle
			(at 3.575 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 249 "unconnected-(U1F-PMUIO1-PadY20)")
			(pinfunction "PMUIO1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "94de0b28-f8f1-4efd-8532-30f44cc222c8")
		)
		(pad "Y21" smd circle
			(at 4.225 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 238 "unconnected-(U1F-PMUPLL_AVDD_1V8-PadY21)")
			(pinfunction "PMUPLL_AVDD_1V8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "89c81208-1dba-4e0f-bf57-809682c2799a")
		)
		(pad "Y22" smd circle
			(at 4.875 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 327 "unconnected-(U1F-GPIO0_A4_U-PadY22)")
			(pinfunction "GPIO0_A4_U")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
			(uuid "c30c3c9e-23a8-48f6-a024-bf7ddc0f0d33")
		)
		(pad "Y23" smd circle
			(at 5.525 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "04005961-c215-4966-b853-ca21b099e315")
		)
		(pad "Y24" smd circle
			(at 6.175 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "27744f32-b940-465e-b7c4-718b2489f183")
		)
		(pad "Y25" smd circle
			(at 6.825 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 173 "unconnected-(U1V-PCIE30_REFCLKP_IN-PadY25)")
			(pinfunction "PCIE30_REFCLKP_IN")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "60c15ea8-e05f-4188-88b3-1b0d656f2a9b")
		)
		(pad "Y26" smd circle
			(at 7.475 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(U1A-AVSS2-PadAA12)")
			(pinfunction "AVSS2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(uuid "b16ba2ea-c782-4455-9c7c-bf445e3ab7c0")
		)
		(pad "Y27" smd circle
			(at 8.125 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 154 "unconnected-(U1T-PCIE20_RXP{slash}SATA2_RXP{slash}QSGMII_RXP_M1-PadY27)")
			(pinfunction "PCIE20_RXP/SATA2_RXP/QSGMII_RXP_M1")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "5365199b-c6e1-4bb8-81cc-fd149b6a5fca")
		)
		(pad "Y28" smd circle
			(at 8.775 3.575)
			(size 0.34 0.34)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 148 "unconnected-(U1T-PCIE20_RXN{slash}SATA2_RXN{slash}QSGMII_RXN_M1-PadY28)")
			(pinfunction "PCIE20_RXN/SATA2_RXN/QSGMII_RXN_M1")
			(pintype "input")
			(solder_mask_margin 0.102)
			(uuid "4e7fd48e-2b1b-4a4c-9c44-1435faea3a50")
		)
		(embedded_fonts no)
	)
	(embedded_fonts no)
)
