
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "RK809-1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -22.86 76.962 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "RK809-1" (id 1) (at -22.86 -78.74 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "RK809-1:QFN35P700X700X80-69N" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "Fuzhou Rockchip Electronics Co" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "0.8mm" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "Package" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/RK809-1/Fuzhou+Rockchip+Electronics+Co/view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "IPC 7351B" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "1.01" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/RK809-1/Fuzhou+Rockchip+Electronics+Co/view-part/?ref=snap" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "RK809-1" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            Complex power-management integrated circuit (PMIC) integrated\nCODEC for multi-core system applications\n                        \n" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SNAPEDA_PN" "RK809-1" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "Not in stock" (id 15) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Rockchip" (id 16) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "RK809-1_0_0"
      (rectangle (start -22.86 -76.2) (end 22.86 76.2)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 27.94 17.78 180.0) (length 5.08)
        (name "SW2"
          (effects (font (size 1.016 1.016)))
        )
        (number "9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -27.94 38.1 0) (length 5.08)
        (name "SDA"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input clock (at -27.94 35.56 0) (length 5.08)
        (name "SCL"
          (effects (font (size 1.016 1.016)))
        )
        (number "1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -40.64 180.0) (length 5.08)
        (name "LDO7"
          (effects (font (size 1.016 1.016)))
        )
        (number "3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 -38.1 180.0) (length 5.08)
        (name "VCC7"
          (effects (font (size 1.016 1.016)))
        )
        (number "4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -43.18 180.0) (length 5.08)
        (name "LDO8"
          (effects (font (size 1.016 1.016)))
        )
        (number "5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -45.72 180.0) (length 5.08)
        (name "LDO9"
          (effects (font (size 1.016 1.016)))
        )
        (number "6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at -27.94 53.34 0) (length 5.08)
        (name "INT"
          (effects (font (size 1.016 1.016)))
        )
        (number "7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at 27.94 15.24 180.0) (length 5.08)
        (name "FB2"
          (effects (font (size 1.016 1.016)))
        )
        (number "8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 30.48 180.0) (length 5.08)
        (name "VCC1"
          (effects (font (size 1.016 1.016)))
        )
        (number "11"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 27.94 180.0) (length 5.08)
        (name "SW1"
          (effects (font (size 1.016 1.016)))
        )
        (number "12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at 27.94 25.4 180.0) (length 5.08)
        (name "FB1"
          (effects (font (size 1.016 1.016)))
        )
        (number "13"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input clock (at -27.94 27.94 0) (length 5.08)
        (name "LRCLK"
          (effects (font (size 1.016 1.016)))
        )
        (number "14"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input clock (at -27.94 30.48 0) (length 5.08)
        (name "BCLK"
          (effects (font (size 1.016 1.016)))
        )
        (number "15"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input clock (at -27.94 25.4 0) (length 5.08)
        (name "MCLK"
          (effects (font (size 1.016 1.016)))
        )
        (number "16"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 20.32 0) (length 5.08)
        (name "SDI"
          (effects (font (size 1.016 1.016)))
        )
        (number "17"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at -27.94 17.78 0) (length 5.08)
        (name "SDO/PDMDATA"
          (effects (font (size 1.016 1.016)))
        )
        (number "18"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output clock (at -27.94 22.86 0) (length 5.08)
        (name "PDMCLK"
          (effects (font (size 1.016 1.016)))
        )
        (number "19"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -20.32 180.0) (length 5.08)
        (name "LDO3"
          (effects (font (size 1.016 1.016)))
        )
        (number "20"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -17.78 180.0) (length 5.08)
        (name "LDO2"
          (effects (font (size 1.016 1.016)))
        )
        (number "21"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 -12.7 180.0) (length 5.08)
        (name "VCC5"
          (effects (font (size 1.016 1.016)))
        )
        (number "22"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -15.24 180.0) (length 5.08)
        (name "LDO1"
          (effects (font (size 1.016 1.016)))
        )
        (number "23"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 10.16 180.0) (length 5.08)
        (name "VCC3"
          (effects (font (size 1.016 1.016)))
        )
        (number "24"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 7.62 180.0) (length 5.08)
        (name "SW3"
          (effects (font (size 1.016 1.016)))
        )
        (number "25"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 5.08 180.0) (length 5.08)
        (name "VBUCK3"
          (effects (font (size 1.016 1.016)))
        )
        (number "26"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at 27.94 2.54 180.0) (length 5.08)
        (name "FB3"
          (effects (font (size 1.016 1.016)))
        )
        (number "27"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -27.94 180.0) (length 5.08)
        (name "LDO4"
          (effects (font (size 1.016 1.016)))
        )
        (number "28"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -30.48 180.0) (length 5.08)
        (name "LDO5"
          (effects (font (size 1.016 1.016)))
        )
        (number "29"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 -25.4 180.0) (length 5.08)
        (name "VCC6"
          (effects (font (size 1.016 1.016)))
        )
        (number "30"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -33.02 180.0) (length 5.08)
        (name "LDO6"
          (effects (font (size 1.016 1.016)))
        )
        (number "31"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -63.5 180.0) (length 5.08)
        (name "SPKP_OUT"
          (effects (font (size 1.016 1.016)))
        )
        (number "32"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 -60.96 180.0) (length 5.08)
        (name "VCC_SPK_HP"
          (effects (font (size 1.016 1.016)))
        )
        (number "33"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -66.04 180.0) (length 5.08)
        (name "SPKN_OUT"
          (effects (font (size 1.016 1.016)))
        )
        (number "34"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 63.5 180.0) (length 5.08)
        (name "VCC_CPVSS"
          (effects (font (size 1.016 1.016)))
        )
        (number "35"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 7.62 0) (length 5.08)
        (name "CPN"
          (effects (font (size 1.016 1.016)))
        )
        (number "36"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 5.08 0) (length 5.08)
        (name "CPP"
          (effects (font (size 1.016 1.016)))
        )
        (number "37"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 66.04 180.0) (length 5.08)
        (name "VCC_CPVDD"
          (effects (font (size 1.016 1.016)))
        )
        (number "38"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -50.8 180.0) (length 5.08)
        (name "HPL_OUT"
          (effects (font (size 1.016 1.016)))
        )
        (number "39"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at 27.94 -55.88 180.0) (length 5.08)
        (name "HP_SNS"
          (effects (font (size 1.016 1.016)))
        )
        (number "40"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -53.34 180.0) (length 5.08)
        (name "HPR_OUT"
          (effects (font (size 1.016 1.016)))
        )
        (number "41"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 0.0 0) (length 5.08)
        (name "MICIN"
          (effects (font (size 1.016 1.016)))
        )
        (number "42"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 -2.54 0) (length 5.08)
        (name "MICIP"
          (effects (font (size 1.016 1.016)))
        )
        (number "43"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 71.12 180.0) (length 5.08)
        (name "VCC_1P8A"
          (effects (font (size 1.016 1.016)))
        )
        (number "44"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 60.96 180.0) (length 5.08)
        (name "VCC_RTC"
          (effects (font (size 1.016 1.016)))
        )
        (number "45"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 -22.86 0) (length 5.08)
        (name "VREF"
          (effects (font (size 1.016 1.016)))
        )
        (number "46"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 -71.12 180.0) (length 5.08)
        (name "GNDREF"
          (effects (font (size 1.016 1.016)))
        )
        (number "47"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 68.58 180.0) (length 5.08)
        (name "VCC_1P8D"
          (effects (font (size 1.016 1.016)))
        )
        (number "48"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 55.88 0) (length 5.08)
        (name "SLEEP"
          (effects (font (size 1.016 1.016)))
        )
        (number "49"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 -7.62 0) (length 5.08)
        (name "XIN"
          (effects (font (size 1.016 1.016)))
        )
        (number "50"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at -27.94 -10.16 0) (length 5.08)
        (name "XOUT"
          (effects (font (size 1.016 1.016)))
        )
        (number "51"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 43.18 0) (length 5.08)
        (name "~{PWRON}"
          (effects (font (size 1.016 1.016)))
        )
        (number "52"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 40.64 180.0) (length 5.08)
        (name "SW5"
          (effects (font (size 1.016 1.016)))
        )
        (number "53"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 43.18 180.0) (length 5.08)
        (name "VCC9"
          (effects (font (size 1.016 1.016)))
        )
        (number "54"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 35.56 180.0) (length 5.08)
        (name "SWOUT1"
          (effects (font (size 1.016 1.016)))
        )
        (number "55"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 73.66 180.0) (length 5.08)
        (name "BATDIV"
          (effects (font (size 1.016 1.016)))
        )
        (number "56"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 48.26 180.0) (length 5.08)
        (name "SWOUT2"
          (effects (font (size 1.016 1.016)))
        )
        (number "58"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at 27.94 -7.62 180.0) (length 5.08)
        (name "FB4"
          (effects (font (size 1.016 1.016)))
        )
        (number "64"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 12.7 0) (length 5.08)
        (name "EXT_EN"
          (effects (font (size 1.016 1.016)))
        )
        (number "60"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 55.88 180.0) (length 5.08)
        (name "VDC"
          (effects (font (size 1.016 1.016)))
        )
        (number "61"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 -17.78 0) (length 5.08)
        (name "SNSN"
          (effects (font (size 1.016 1.016)))
        )
        (number "63"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 -15.24 0) (length 5.08)
        (name "SNSP"
          (effects (font (size 1.016 1.016)))
        )
        (number "62"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at 27.94 38.1 180.0) (length 5.08)
        (name "FB5"
          (effects (font (size 1.016 1.016)))
        )
        (number "59"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 -5.08 180.0) (length 5.08)
        (name "SW4"
          (effects (font (size 1.016 1.016)))
        )
        (number "65"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 48.26 0) (length 5.08)
        (name "RESETB"
          (effects (font (size 1.016 1.016)))
        )
        (number "67"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output clock (at -27.94 50.8 0) (length 5.08)
        (name "CLK32K"
          (effects (font (size 1.016 1.016)))
        )
        (number "68"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 -73.66 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "69"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 20.32 180.0) (length 5.08)
        (name "VCC2"
          (effects (font (size 1.016 1.016)))
        )
        (number "10"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 -2.54 180.0) (length 5.08)
        (name "VCC4"
          (effects (font (size 1.016 1.016)))
        )
        (number "66"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 50.8 180.0) (length 5.08)
        (name "VCC8"
          (effects (font (size 1.016 1.016)))
        )
        (number "57"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)